*********************************************************
*  Product: Intel(R) Chipset Software Installation Utility
*  Release: Beta 3
*  Version: 6.1.0.1006
*  Target Chipset#: Mobile Intel(R) 915GM/PM/GMS/910GML
*  Date: April 08, 2004 
*********************************************************

NOTE: For the list of supported chipsets, please refer to 
      the Release Notes

*********************************************************
*  CONTENTS OF THIS DOCUMENT
*********************************************************
This document contains the following sections:

1.  Overview
2.  System Requirements
3.  Contents of the Distribution Package
4.  List of Available Command Line Flag Options 
5.  Contents of the Extracted Files
6.  Installing the Software in Interactive Mode
7.  Installing the Software in Silent Mode
8.  Installing the INF Files Prior to OS Installation
    8A. Installing the Windows* 98SE/Windows* Me 
        INF Files Prior to OS Installation
    8B. Installing the Windows* 2000 INF Files Prior
        to OS Installation
    8C. Installing the Windows* XP INF Files Prior
        to OS Installation
    8D. Installing the Windows Server* 2003 INF Files 
        Prior to OS Installation
9.  Installing the INF Files After OS Installation
    9A. Installing the Windows* 98SE/Windows* Me INF 
        Files After OS Installation
    9B. Installing the Windows* 2000 INF Files After
        OS Installation
    9C. Installing the Windows* XP INF Files After
        OS Installation 
    9D. Installing the Windows Server* 2003 INF Files 
        After OS Installation
10. Verifying Installation of the Software and 
    Identifying the Software Version Number
11. Troubleshooting


************************************************************
* 1.  OVERVIEW
************************************************************
The Intel(R) Chipset Software Installation Utility installs
Windows* INF files to the target system. These files outline
to the operating system how to configure the Intel(R) chipset 
components in order to ensure that the following features 
function properly:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66/ATA100 Storage Support
   - SATA Storage Support
   - USB Support
   - Identification of Intel(R) Chipset Components in 
     the Device Manager

This software can be installed in three modes: Interactive,
Silent and Unattended Preload. Interactive Mode requires 
user input during installation; Silent Mode and Unattended 
Preload do not.  

This software also offers a set of command line flags, 
which provide additional installation choices. The command 
line flags are not case sensitive. Refer to Section 4 for 
detailed descriptions of these flags.

Important Note:
The Intel(R) Chipset Software Installation Utility is 
distributed in two formats: self extracting .EXE files
(INFINST_xxx.EXE) or compressed .ZIP files (INFINST_xxx.ZIP). 
Depending on which distribution format is being executed, the 
command-line syntax may differ. Refer to Section 4 for more 
details. 


************************************************************
* 2.  SYSTEM REQUIREMENTS 
************************************************************
1.  Please refer to the Release Notes to view the list of 
    chipsets that the software included with this distribution 
    package is designed to operate with.

2.  One of the following operating systems must be 
    fully installed and running on the system
    before installing this software:

    Windows* 98SE	  4.10.2222  (Original Release)
    Windows* Me  	  4.90.3000  (Original Release)
    Windows* 2000	  5.00.2195  (Original Release)
    Windows* XP  	  5.10.2600  (Original Release)
    Windows Server* 2003  5.20.3790  (Original Release)

    To verify which operating system has been installed onto 
    the target system, follow the steps below:

    a.  Click on Start.
    b.  Select Settings.
    c.  Select Control Panel.
    d.  Double-click on the System icon.
    e.  Click on the General system properties tab.
    f.  Verify which OS has been installed by reading
        the System information.
                              
3.  It is recommended that the software be installed on 
    systems with at least 32MB of system memory when using 
    Windows* 98SE and Windows* Me. Windows* 2000 and Windows* XP
    require at least 64MB of system memory.

4.  It is recommended that there be a minimum of 5MB of hard
    disk space on the system in order to install this software.

5.  Check the System Requirements. The operating system 
    must be fully installed and running on the system before
    running this software.

6.  Close any running applications to avoid installation problems.

7.  It is recommended that the Intel(R) Chipset Software 
    Installation Utility be installed onto the target system 
    prior to the installation of other drivers.

Please check with the system provider to determine which 
operating system and Intel(R) chipset are used in the system.


************************************************************
* 3.  CONTENTS OF THE DISTRIBUTION PACKAGE
************************************************************
The Intel(R) Chipset Software Installation Utility package 
contains the following items:

    File(s)       
    -------
    INFINST_xxx.EXE -or- INFINST_xxx.ZIP
    README.TXT, RELEASE_xxx.HTM

   *** NOTE:  Only the files that reference the currently 
              detected devices are copied to the system.
	      
              If the -A option is exercised, the files are
              not copied to the <Windows>\INF directory.
              Refer to Section 4 for more information.  

                                       
************************************************************
* 4.  LIST OF AVAILABLE COMMAND LINE FLAG OPTIONS
************************************************************
The Intel(R) Chipset Software Installation Utility supports  
several command line flags for various installation options. 
All command line flags and parameters must be separated by a 
space, except for the language code after the '-L' flag.

Due to the different distribution formats available for the
Intel(R) Chipset Software Installation Utility, the command
line flag syntax may vary:

1. Self-Extracting .EXE Distribution:
      When installing this software using the .EXE 
      distribution, an extra '-A' must be appended to the 
      INFINST_xxx.EXE program call (i.e. INFINST_ENU.EXE -A) 
      in order to successfully pass command line flags.

   NOTE: The extra '-A' flag for the self-extracting .EXE 
         package is different from the '-A' command line flag 
         option described under Compressed .ZIP Distribution.        

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
          
               INFINST_ENU.EXE -A -A (optional -P)

2. Compressed .ZIP Distribution:
      When installing this software using the .ZIP distribution, 
      use the command line flags exactly as discribed below.

      Example: To extract INF files using the '-A' flag 
               described below, the installation program 
               should be invoked as follows:  
                        
               SETUP.EXE -A (optional -P)

Below is a list of all the available command line flags that
may be used with the program call.  Note that the '-L' and 
the '-S' flags MUST be specified at the end of the command 
line flag list.

Flag            Description
----            -----------
-?              Displays the list of available command line 
                flags. This flag works in Interactive Mode only.  

-A              Extracts the INF files and Readme to either 
                "C:\Program Files\Intel\InfInst" or the
                <Installation Path> directory specified using 
                the '-P' flag. The software will NOT install 
                these INF files to the system. This flag can 
                be combined only with the '-P' flag. All other
                options will be ignored if the '-A' flag is 
                specified. This flag works in either Silent 
                Mode or Interactive Mode.

-B              Automatically reboots the system after 
                installation. This flag is ignored if '-A' flag
                is specified. This flag works in either Silent 
                Mode or Interactive Mode.

-H<mode>
                Enables DMA Mode for an IDE device.

-L<LangCode>
                Forces the InstallShield* user interface to 
                display the specified language during setup.  
                Note that there should be NO spaces between 
                '-L' and the 4-digit language code (see below). 
                This flag and the '-S' flag must be placed at 
                the end of the command line flag list. This 
                flag works in Interactive Mode only.

-NOLIC
                Disables the license agreement dialog box during
                installation. This parameter works in Interactive
                Mode only.

-NOREAD
                Disables the Readme display during installation. 
                This flag works in Interactive Mode only.

-NOWEL
                Disables the welcome screen during installation. 
                This flag works in Interactive Mode only.

-OVER ALL	
                Updates ALL INF drivers even if third party
                drivers are currently installed. This flag 
                works in Interactive Mode only.

-OVER FWH
                Updates the security drivers even if a third 
                party security driver is currently installed. 
                This flag works in Interactive Mode only.

-OVER IDE	
                Updates the storage drivers even if a third
                party storage driver is currently installed. 
                This flag works in Interactive Mode only.

-OVER SMB	
                Updates the LAN drivers even if third party LAN 
                drivers are currently installed. This flag works 
                in Interactive Mode only.

-P <Installation Path>   
                Specifies the hard disk location to which the 
                INF program files are copied. If this flag is 
                not specified at the command line, the 
                <Installation Path> directory is as follows: 
                
                   C:\Program Files\Intel\INFInst
                
               	If this flag is used without the '-A' option, 
               	only the Readme will be copied to 
               	<Installation Path>. The directory name can 
               	include spaces, but then a pair of double quotes 
               	(") must enclose the directory name. This flag 
               	works in either Silent Mode or Interactive Mode.

-S              Runs the Installer in Silent Mode (no user 
                interface is displayed). This flag and the
                '-L' flag must be placed at the end of the 
                command line flag list.

                
-SKIP<DevID>
                Suppresses the installation of one or more 
                devices.This flag works in either Silent Mode 
            	or Interactive Mode. 

-INTELIDE       
               	Installs the INTELIDE.SYS instead of the default 
               	PCI storage driver, PCIIDE.SYS. This flag only 
               	operates on Windows* 2000, Windows* XP, 
               	and Windows Server* 2003. On other operating
               	systems, this flag will be ignored and the default
               	PCI storage driver, PCIIDE.SYS, will be installed. 
               	This flag works in either Silent Mode or Interactive 
               	Mode. 

Below are the language codes used with the '-L' flag:

    Language         		<LangCode>
    --------         		----------
    Chinese (Simplified)  	0804    
    Chinese (Traditional) 	0404
    Czech             		0005
    Danish            		0006
    Dutch              		0013
    English (United States)	0009
    Finnish            		000B
    French (Canada)     	0C0C
    French (Standard)     	040C
    German            		0007
    Greek              		0008
    Hungarian         		000E
    Italian            		0010
    Japanese           		0011
    Korean             		0012
    Norwegian          		0014
    Polish            		0015
    Portuguese (Brazil)  	0416
    Portuguese (Standard) 	0816
    Russian            		0019
    Spanish           		000A
    Swedish               	001D
    Thai               		001E
    Turkish            		001F


************************************************************
* 5.  CONTENTS OF THE EXTRACTED FILES
************************************************************
INF files are copied to the hard disk after running the Intel(R)
Chipset Software Installation Utility executable with an '-A' 
flag (i.e., "INFINST_ENU.EXE -A -A" or "SETUP.EXE -A"). The 
location of the INF files depends on whether a '-P' flag is 
specified along with the '-A' flag:

1.  If a '-P' flag is not specified, then the INF files are 
    copied to the following directory:  
       "C:\Program Files\Intel\INFINST"
2.  If a '-P' flag is specified, then the INF files are copied 
    to the location listed immediately after the '-P' flag.  

    Refer to Section 4 for more information on flag usage.

After INF file extraction, the INF files and components are 
copied to the <INF Extract Directory>. These files and 
components are categorized according to the Intel(R) Chipset 
types. The following table summarizes the locations of the 
INF files by chipsets:

   NOTE: The INF files are designed to update only devices
         not supported by the corresponding operating system.

   NOTE: "<INF Extract Directory>" is abbreviated "<IED>" in 
   	 the remainder of this section.

For each subdirectory of <IED> (e.g., ICH, ICH2, etc), 
the INF files are further classified according to 
the operating systems they are designed for:

   Win98SE\   --->  Contains INF files designed for
                     Windows* 98SE ONLY.
   Win2000\   --->  Contains INF files designed for
                     Windows* 2000 ONLY.
   WinMe\     --->  Contains INF files designed for
                     Windows* Me ONLY.
   WinXP\     --->  Contains INF files designed for
                     Windows* XP ONLY.
   Win2003\   --->  Contains INF files designed for
                     Windows Server* 2003 ONLY.

NOTE: INFPrelo.INF makes a CUSTOM.INF template that installs 
the INF files for Intel(R) chipsets during operating system 
setup. OEMs can incorporate this file into the Setup directory 
for the OEM Preload Kit. (Refer to Section 8 for more details.)


************************************************************
* 6.  INSTALLING THE SOFTWARE IN INTERACTIVE MODE
************************************************************
1.  Verify that all system requirements have been met as 
     described in Section 2 above.

2.  Run the InstallShield* installation program:
     Self-extracting .EXE distribution: INFINST_xxx.EXE
     Compressed .ZIP distribution: SETUP.EXE

3.  You will be prompted to agree to the license agreement.  
     If you do not agree, the installation program will exit 
     before extracting any files.
    
4.  Once the operating system reboots, follow the on-screen 
     instructions and accept default settings to complete the 
     setup.


************************************************************
* 7.  INSTALLING THE SOFTWARE IN SILENT MODE
************************************************************
1.  Verify that all system requirements have been met as 
     described in section 2.

2.  Run the InstallShield* installation program:
     For silent install with auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_xxx.EXE -a -b -s
       Compressed .ZIP distribution:
       SETUP.EXE -b -s
    - or -
     For silent install without auto-reboot:
       Self-extracting .EXE distribution: 
       INFINST_xxx.EXE -a -s
       Compressed .ZIP distribution: SETUP.EXE -s

3.  The utility will perform the necessary updates and 
     record the installation status in the following system 
     registry key:
        HKEY_LOCAL_MACHINE\Software\Intel\INFInst

4.  If the utility was invoked with the "-b" flag, the 
     system will automatically reboot if the update was
     successful.

    NOTE: The system MUST be rebooted for all device 
    updates to take effect.

5.  To determine whether the install was successful, verify 
     the "install" value in the registry key specified in 
     Step 3.

6.  In Silent Mode the utility will not display the license
     agreement. When using Silent Mode the license agreement,
     license.txt, will be placed in the following folder:
     Program Files/Intel/INFInst folder.
     Please read this agreement.

    The following table describes the various parameters:

	Name		Type	Data		Description
	-----		----	----		-----------
	"install"      	String 	"success"      	The installation was 
						successful.

				"fail"		The installation was 
						not successful.
						No INF files were 
						copied to the system.

       	"reboot"       	String	"Yes"		A reboot is required to 
						complete the installation.

				"No"		No reboot is required 
						to complete the 
						installation.

       	"version"      	String 	<varies>       	Current version number 
						of the Intel(R) Chipset 
						Software Installation 
						Utility


************************************************************
* 8.  INSTALLING THE INF FILES PRIOR TO OS INSTALLATION
************************************************************
    This procedure requires a minimum of 5MB of hard disk space. 
    It is important to make sure there is enough disk space 
    before beginning the copy process. Copy the operating system 
    installation files from the setup directory to a directory
    on the hard disk. This can be done by opening 'My Computer', 
    right-clicking on the correct drive, and selecting 'Properties'.
    The directories shall be referred to as follows:


      Windows* 98SE	: <WIN98SE Setup Directory>
      Windows* Me	: <WINMe Setup Directory>
      Windows* 2000	: <WIN2000 Setup Directory>
      Windows* XP	: <WINXP Setup Directory>
      Windows Server* 2003 : <WIN2003 Setup Directory>
        

************************************************************
* 8A.  INSTALLING THE WINDOWS* 98SE/WINDOWS* ME 
*      INF FILES PRIOR TO OS INSTALLATION
************************************************************
NOTE: The Windows* 98SE or Windows* Me OEM Preload Kit 
      distribution CD contains a setup directory with all the 
      base operating system setup files (*.CAB) and the 
      installation program (SETUP.EXE).

The name of the directory may vary depending on the 
distribution CD (e.g., \WIN98SE\).   

1.   If you are preloading Windows* 98SE, copy the 
     Windows* 98SE INF files from
     <INF Extract Directory>\XXXX\Win98SE to the 
     setup directory.
       -or-
     If you are preloading Windows* Me, copy the 
     Windows* Me INF files from
     <INF Extract Directory>\XXXX\WinMe to the 
     setup directory.  
    
     NOTE: XXXX is the directory name for the chipset of 
     interest. Refer to Section 8 for more details.

2.  Run SETUP.EXE to install Windows* 98SE or Windows* Me.


************************************************************
* 8B.  INSTALLING THE WINDOWS* 2000 INF FILES PRIOR TO
*      OS INSTALLATION
************************************************************
NOTE: The Windows* 2000 OEM Preload Kit distribution CD
      contains a setup directory with all the base operating
      system setup files and installation programs 
      (WINNT.EXE and WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows* 2000 INF files from 
    <INF Extract Directory>\XXXX\Win2000 to the directory
    created in Step 1 above:

       <WIN2000 Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WIN2000 Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows* 2000 INF files and the catalog files 
    (.CAT) from <INF Extract Directory>\XXXX\Win2000 to the 
    directory created in Step 4 above:

       <WIN2000 Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

5.  Either modify the default Windows* 2000 installation
    answer file, UNATTEND.TXT, located in <WIN2000 Setup 
    Directory>, or create a customized answer file. The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Software Installation utility files is available: 
    <INF Extract Directory>\XXXX\Win2000\INFAnswr.TXT
    
    For more information about Windows* 2000 answer files 
    and unattended installations, please refer to the 
    Microsoft* Windows* 2000 Guide to Unattended Setup. 
    If you are a computer manufacturer, refer to the 
    Microsoft Windows* 2000 OEM Preinstallation Kit (OPK) 
    User Guide for more information about the \$OEM$ folder. 
    Otherwise, refer to the Microsoft Windows* 2000 Deployment 
    Guide.

6.  Run "WINNT.EXE /u:<answer file name> /s:<WIN2000 Setup 
    Directory>" to install Windows* 2000.


************************************************************
* 8C.  INSTALLING THE WINDOWS* XP INF FILES PRIOR TO
*      OS INSTALLATION
************************************************************
NOTE: The Windows* XP OEM Preload Kit distribution CD contains 
      a setup directory with all the base operating system 
      setup files and installation programs (WINNT.EXE and
      WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WINXP Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows* XP INF files from 
    <INF Extract Directory>\XXXX\WinXP to the directory
    created in Step 1 above:

       <WINXP Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest.  Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WINXP Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows* XP INF files AND the catalog files 
    (.CAT) from <INF Extract Directory>\XXXX\WinXP to the 
    directory created in Step 4 above:

       <WINXP Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

5.  Either modify the default Windows* XP installation
    answer file, UNATTEND.TXT, located in <WINXP Setup 
    Directory>, or create a customized answer file.  The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Software Installation utility files is available: 
    <INF Extract Directory>\XXXX\WinXP\INFAnswr.TXT
    
    If you are a computer manufacturer, refer to the Microsoft* 
    Windows* XP Guide to Unattended Setup for more information 
    about Windows* XP answer files and unattended installations. 
    For more information about the \$OEM$ folder, refer to the 
    Microsoft Windows* XP OEM Preinstallation Kit (OPK) 
    User Guide. If you are not a manufacturer, refer to the Microsoft 
    Windows* XP Deployment Guide.

6.  Run "WINNT.EXE /u:<answer file name> /s:<WINXP Setup 
    Directory>" to install Windows* XP.


************************************************************
* 8D.  INSTALLING THE WINDOWS SERVER* 2003 INF FILES PRIOR 
*      TO OS INSTALLATION
************************************************************
NOTE: The Windows Server* 2003 OEM Preload Kit distribution 
      CD contains a setup directory with all the base operating
      system setup files and installation programs (WINNT.EXE 
      and WINNT32.EXE).  

The name of the directory may vary depending on the 
distribution CD (e.g., \I386\).

1.  Create the following directory structure under the 
    <WIN2003 Setup Directory>: 

       \$OEM$\$$\INF

2.  Copy the Windows Server* 2003 INF files from 
    <INF Extract Directory>\XXXX\Win2003 to the directory
    created in Step 1 above:

       <WIN2003 Setup Directory>\$OEM$\$$\INF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

3.  Create the following directory structure under the 
    <WIN2003 Setup Directory>: 

       \$OEM$\$1\drivers\IntelINF

4.  Copy the Windows Server* 2003 INF files and the catalog 
    files (.CAT) from <INF Extract Directory>\XXXX\Win2003 
    to the directory created in Step 3 above:

       <WIN2003 Setup Directory>\$OEM$\$1\drivers\IntelINF

    NOTE: XXXX is the directory name for the chipset of 
          interest. Refer to Section 8 for more details.

5.  Either modify the default Windows Server* 2003 installation
    answer file, UNATTEND.TXT, located in <WIN2000 Setup 
    Directory>, or create a customized answer file. The
    answer file must include the following information:
   
       [Unattended]
       OemPreinstall = Yes
       OemPnPDriversPath="drivers\IntelINF"

    A sample answer file for preloading the Intel(R) Chipset
    Software Installation utility files is available: 
    <INF Extract Directory>\XXXX\Win2003\INFAnswr.TXT
    
    For more information about Windows Server* 2003 answer 
    files and unattended installations, please refer to the 
    Microsoft Windows Server* 2003 Guide to Unattended Setup.
    If you are a computer manufacturer, refer to the Microsoft 
    Windows Server* 2003 OEM Preinstallation Kit (OPK) User 
    Guide for more information about the \$OEM$ folder. 
    Otherwise, refer to the Microsoft Windows Server* 2003 
    Deployment Guide.


6.  Run "WINNT.EXE /u:<answer file name> /s:<WIN2003 Setup 
    Directory>" to install Windows* 2000.


************************************************************
* 9.  INSTALLING THE INF FILES AFTER OS INSTALLATION
************************************************************

************************************************************
* 9A.  INSTALLING THE WINDOWS* 98SE/WINDOWS* 
*      ME INF FILES AFTER OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms are already supported by 
Windows* 98SE and Windows* Me, so it may not be necessary 
to use the INF files provided by this software to update 
these operating systems.

The following steps describe the installation process for
the Windows* 98 Second Edition and Windows* Me INF files.  
You may need to repeat these steps to update all Intel(R) 
chipset devices not supported by these operating systems.

    1.  Depending on the operating system you intend to 
        update, copy the contents of one of the following 
        directories to the root directory of the floppy 
        disk (A:\).

       For Windows* 98SE: 
                 <INF Extract Directory>\XXXX\Win98SE
       For Windows* Me: 
                 <INF Extract Directory>\XXXX\WinME
     
        NOTE: XXXX is the directory name for the chipset of
              interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select Control Panel.
    6.  Double click on the System icon.
    7.  Click on the Device Manager tab.
    8.  Click on the View Devices by Connection button.
    9.  Click on Plug and Play BIOS, or Advanced Configuration
        and Power Interface (ACPI) BIOS.
        NOTE: Only one of the above items will be 
              displayed for a given system.
    10. Click on PCI bus.
    11. Click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    12. Click on the Remove button at the bottom of the 
        window.
    13. If more than one Intel(R) chipset device needs 
        updating, go to Step 11 to remove more devices.
    14. When prompted to reboot the system, select Yes.
    15. Reboot the system.
    16. The Windows operating system will launch the Add
        New Hardware Wizard.
        Select Next in the dialog box that states:
            "This wizard searches for new drivers for:"
    17. Ensure that the following choice is selected:
            Search for the best driver for your device 
            (Recommended)
    18. Select Next.
    19. Insert the floppy containing the .INF files into
        the floppy drive.
    20. Ensure that the following choice is selected:
            Floppy disk drives
    21. If the .INF files are not located in the root 
        directory of the floppy disk, also select the 
        "Specify a location" and enter the path to the .INF 
        files needed to update this operating system.
    22. Select Next.
    23. The Windows operating system should report that
        the driver has been found and that it is "now 
        ready to install the best driver for this 
        device."
    24. Select Next.
    25. Select Finish.
    26. The Windows operating system may prompt you to 
        install additional drivers if more than one device
        was removed during Steps 11 through 13. Follow the 
        same procedure to install the remaining Intel(R) 
        chipset devices.
    27. Reboot the system when prompted to do so.


************************************************************
* 9B.  INSTALLING THE WINDOWS* 2000 INF FILES AFTER OS 
*      INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows* 2000, so it may not be necessary to use the INF 
files provided by this software to update Windows* 2000.

The following steps describe the installation process of
the Windows* 2000 INF files. You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows* 2000.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\Win2000 
        directory to the root directory of the floppy disk
        (A:\).
        
        NOTE: XXXX is the directory name for the chipset 
              of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
        Multiprocessor PC.
        NOTE:  Only one of the above items will be 
               displayed for a given system.
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows* 2000 will launch the Upgrade Device Driver 
        Wizard. Select Next.
    17. Ensure that the following choice is selected:
            Search for a suitable driver for my device 
            (recommended)
    18. Insert the floppy containing the Windows* 2000 INF 
        files into the floppy drive.
    19. Select Next.
    20. Windows* 2000 will list locations from where the 
        updated driver file can be found.  Ensure that the 
        following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows* 2000 should report that a driver has been
        found: (The detected device name will be displayed.)
        Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.

************************************************************
* 9C.  INSTALLING THE WINDOWS* XP INF FILES AFTER OS 
*      INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows* XP so it may not be necessary to use the INF 
files provided by this software to update Windows* XP.

The following steps describe the installation process of
the Windows* XP INF files. You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows* XP.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\WinXP 
        directory to the root directory of the floppy disk
        (A:\).
        
        NOTE: XXXX is the directory name for the chipset 
              of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
        Multiprocessor PC.
        NOTE: Only one of the above items will be 
              displayed for a given system.
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows* XP will launch the Upgrade Device Driver 
        Wizard. Select Next.
    17. Ensure that the following choice is selected:
            Search for a suitable driver for my device 
            (recommended)
    18. Insert the floppy containing the Windows* XP INF 
        files into the floppy drive.
    19. Select Next.
    20. Windows* XP will list locations from where the 
        updated driver file can be found.  Ensure that the 
        following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows* XP should report that a driver has been
        found: (The detected device name will be displayed.)
        Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.


************************************************************
* 9D.  INSTALLING THE WINDOWS SERVER* 2003 INF FILES AFTER 
*      OS INSTALLATION
************************************************************
Some Intel(R) chipset platforms already are supported by 
Windows Server* 2003 so it may not be necessary to use the INF 
files provided by this software to update Windows Server* 2003.

The following steps describe the installation process of
the Windows* XP INF files.  You may need to repeat these 
steps to update all Intel(R) chipset devices not supported
by Windows Server* 2003.

    1.  Copy the contents of the 
        <INF Extract Directory>\XXXX\Win2003
        directory to the root directory of the floppy disk
        (A:\).
        
        NOTE: XXXX is the directory name for the chipset 
              of interest. Refer to Section 8 for more details.
              
    2.  Close all programs currently running on the system.
    3.  Click on Start.
    4.  Select Settings.
    5.  Select the Control Panel.
    6.  Double-click on the System icon.
    7.  Click on the Hardware tab.
    8.  Click on the Device Manager button.
    9.  Select "Devices by connection" under the View menu.
    10. Click on MPS Uniprocessor PC -OR- MPS 
        Multiprocessor PC.
        NOTE: Only one of the above items will be 
              displayed for a given system.
    11. Click on PCI bus.
    12. Right-click on the line containing the description
            PCI standard host CPU bridge
            -or-
            PCI standard ISA bridge
            -or-
            PCI standard PCI-to-PCI bridge
            -or- 
            PCI System Management Bus
            -or- 
            Standard Dual PCI IDE Controller
            -or-
            Standard Universal PCI to USB Host Controller
            (This line will be selected.)
    13. Select Properties from the pull-down menu.
    14. Click on the Driver tab.
    15. Click on the Update Driver button.
    16. Windows Server* 2003 will launch the Upgrade Device 
        Driver Wizard. Select Next.
    17. Ensure that the following choice is selected: Search
    	for a suitable driver for my device (recommended)
    18. Insert the floppy containing the Windows Server* 2003 
	INF files into the floppy drive.
    19. Select Next.
    20. Windows Server* 2003 will list locations from where the 
        updated driver file can be found. Ensure that the 
        following choice is selected: Floppy disk drives
    21. Select Next.
    22. Windows Server* 2003 should report that a driver has 
	been found: (The detected device name will be displayed.)
        Select Next.            
    23. Select Finish.
    24. Reboot the system when prompted to do so.

************************************************************
* 10.	IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The version numbers displayed by Device Manager for a given 
device may not be the same as the Intel(R) Chipset Software 
Installation Utility version.  
 
The correct version number is shown at the top of this readme 
file.


************************************************************
* 11.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements in Section 2 above 
have been satisfied.

Issue:	    At the end of executing the Chipset Software 
	    Installation Utility, the USB keyboard and mouse
	    will stop functioning. This problem only occurs 
	    when using Windows XP with SP1 on a system configured
	    with a USB keyboard and/or mouse. This condition is 
	    temporary until a system reset.

Solution1:  A recommended fix has been provided by Microsoft
            in Knowlege Base article(822603). For additional 
            information, please refer to the KB article located at
            http://support.microsoft.com/default.aspx?scid=kb;[LN];822603  

	    Please use the following installation procedures: 
                - Windows XP installed with SP1
                - QFE (822603) installed
                - Latest Chipset Utility Software installed.

Solution2:  The command line flag "-Skip <DevID>" can be used 
	    with the Intel(R) Chipset Software Installation 
	    Utility program to cause the USB2 driver not to be 
	    installed. The DevID's for ICH4/ICH5 are 24CD/24DD. 
	    This will cause the USB2 controller to have a yellow 
	    exclamation point in Device Manager (Usually located
	    under Other Devices and identified as "Universal 
	    Serial Bus (USB) Controller"). To install the USB2 
	    driver right-click this entry, select update driver, 
	    and allow the system to install automatically. When
	    completed, nothing more should be required.

Issue:	    After installing the Intel(R) Extreme Graphics Driver 
	    to utilize the integrated graphics capabilities of 
	    the Intel(R) chipset, software support for the AGP 
	    function of the chipset is disabled in systems using 
	    the Windows* 98, Windows* 98SE, and Windows* ME 
	    operating systems.

	    
Solution:   If a user wishes to install an external AGP graphics 
	    card subsequent to installing the Intel(R) Extreme 
	    Graphics Driver on a system using a Windows* 98, 
	    Windows* 98SE, or Windows* Me operating system, the 
	    Intel(R) Chipset Software Installation Utility must 
	    be re-installed to re-enable software support for 
	    AGP functionality. (In addition, the driver associated
	    with the graphics card must also be installed.)

Issue:      System locks up during Device Manager Remove or 
            during restart.


Solution:   System lockup can occur during reboot as a 
            result of several possible system issues.  In 
            the event of system lockup, reboot the machine 
            and view Device Manager.  If devices are listed 
            properly and the system experiences no further 
            problems, then the .INF file restore process was 
            successful. If devices are not configured 
            correctly, try re-running the procedures 
            outlined in Section 3.

            If this does not fix the issue or further issues
            are experienced, reinstall the operating system.

Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files: ESDI_506.pdr

Solution:   Click Browse in the dialog box where this issue
            occurs, locate the <Windows>\System\IOSubsys
            directory. Click OK. The system should be able to
            locate this file in this directory and continue 
            re-enumerating for the new devices.

Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            one of the following files:
 
                  UHCD.SYS
                  USBD.SYS
                  USBHUB.SYS

Solution:   Click Browse in the dialog box where this issue 
	    occurs and locate the following directory:
			
                  <Windows>\System32\drivers 
                  (for Windows* 98SE, Windows* Me)
                  
            Click OK. The system should be able to locate the 
            files in this directory and continue re-enumerating 
            for the new devices.

Issue:      After running the setup program and rebooting 
            the machine, Windows reports that it cannot find 
            the following file: ISAPNP.VXD

Solution:   Click Browse in the dialog box where this issue 
	    occurs and locate the <Windows>\System directory. 
	    Click OK. The system should be able to locate this 
	    file in this directory and continue re-enumerating 
	    for the new devices.

Issue:      After performing the silent install, the 
            HKLM\Software\Intel\InfInst key was not created 
            or the data of the value "install" is not 
            "success".

Solution:   This is caused by one of the following 
            scenarios:
               - The current system does not contain a 
                 supported operating system, or
                 -or-
               - The current system does not contain a 
                 supported chipset.

            Verify that the System Requirements are met as 
            outlined in Section 2.


************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or warranty.  
The Intel(R) SOFTWARE LICENSE AGREEMENT
(OEM / IHV / ISV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel(R) products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty relating 
to sale and/or use of Intel(R) products, including liability 
or warranties relating to fitness for a particular purpose, 
merchantability or infringement of any patent, copyright or 
other intellectual property right.  Intel(R) products are 
not intended for use in medical, life saving, or 
life-sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein.  
Intel reserves the right to make changes to this document at 
any time, without notice.
************************************************************
************************************************************

* Intel is a trademark or registered trademark of Intel Corporation 
  or its subsidiaries in the United States and other countries.
* Other brands and names are the property of their 
  respective owners.

Copyright (c) Intel Corporation, 1997-2004
