 Multi-touch Driver Release Notes

                                           Elo Touch Solutions
                                 670 N McCarthy Blvd, Milpitas, CA 95035

                                        Package Version: v9.2.0.8
                                      Release Date: August 27, 2024

****************************************************************************************************


1.   Special note and Known Issues:

    • Special Microsoft KBs Required for Windows 7 (and Server 2008 R2):
      To enable the SHA-2 support on Windows 7, 3 Microsoft KBs need to be installed prior to
      installing the Elo’s driver package which has been signed with Microsoft’s SHA-2 digital
      signature. Please follow the steps below to install the KBs:

	a. Install KB4490628
	b. Install KB4474419 then reboot
	c. Install KB4534310 then reboot.

	For detailed requirements to enable SHA-2 support on Windows 7, please see the Microsoft
        document:

	https://support.microsoft.com/en-us/help/4472027/2019-sha-2-code-signing-support-requirement-for-windows-and-wsus

    • Windows XP is not supported starting from the MT driver version 8.0.0.

    • For 2521 (PID 0x27) controllers with firmware versions older than 6.2, sometimes the 
      touchscreen does not respond to touches in either the upper or lower 1-inch region of the
      monitor. In that case, the monitor needs to be power cycled, then re-calibrated to restore
      normal touch. If power cycling the monitor is not working, the utility EloCalMgr.exe
      (located in the target installation folder) can be used to reset the controller.  

    • In forced mouse mode, calibration on spanned display mode is not supported.

    • On Windows 10/11 with multiple touch monitors, if a touch-controller does not have a unique
      serial number, the touch-to-display mapping may be lost after swapping its USB port. When
      this happens, please reboot or re-calibrate the monitor.

    • On certain operating systems (Windows 8.1/10/11), during calibration, the calibration targets
      may be shown off position. In this case please check the “Windows Item Size” and make sure it
      is set at 100%.

    • IR Beam Monitoring:After the user dismisses the alert box, it will show up again if touch
      monitor’s USB cable is re-plugged or the Property page of EloConfig is opened again.

    • This feature is not suitable to be used with EloTouchZones, the user may not be able to
      dismiss the alert prompt box if the box happens to be inside an area where touch is disabled.

    • Multi-touch package 6.x (or newer) APIs vs. single-touch 5.x APIs. Applications written with
      Elo's single-touch 5.x APIs will not work with multi-touch 6.x (or newer) installation. These
      applications need to be updated (re-compile and link) in order to work with multi-touch
      package 6.x (or newer).
   
2.  History of Changes:

v3.0.1
 
    • EloMtApi: pre-cal not committed to NVRam.
    • USB driver: pivot test missing drawing segments
    • EloConfig.exe: added command line parameter “/align” to allow video alignment.

v3.0.2

   • Write NVRam is turned off by default (EloOptions.ini).
	
v4.0.1
	
   • Support motherboard beep on Windows 7 (both 32-bit and 64-bit systems).
   • Support optical touch screens: 0x202E-0x06 (dual-touch) and 0x04E7-0x80 (four-touches).
   • Sending user defined Smartset commands (in EloOptions.ini) at system startup or driver loading. 
   • Utility to allow user to define touch enabled areas (EloTouchZones.exe).
   • Position log files in “Elo Touch Systems” folder under “ProgramData”.
   • During calibration, once a monitor is touched, the session should be completed on that monitor.
   • Incorrect Windows Monitor number showed in Property page if the system has un-connected video port.
   • IT2701 sleep/resume fails about 20% of times.
   • EloConfig unwanted popup at system startup.
   • Support pCap touch screen 0xEEF-7200. 

v4.0.2

   • Serial driver: New calibration is not taking effect.
   • Serial driver: After reboot, previous calibration is not applied.
   • Serial driver: Pre-install either legacy serial driver or multi-touch serial driver (not both).

v4.0.3

   • Correct the multi touch mode in Lumio/Optical monitor.
   • Added Windows 8 support.
   • Correct SmartSet timing issue.

v4.5.0

   • Provide touch and video functions for IDS Suite. 
   • Provide option to limit number of touches to one touch set the value of “EnableOneTouch” under 
     section “Setup Options” in EloOptions.ini. Users can use this feature to block multi-touch gestures. 
   • Support 6-touch Optical controller.
   • Support new HID controller (PID 0x27).
   • Bug fix: COACH-3 Calibration window not exiting at end of the calibration session.
   • Provide sample program “EloDrawMultiMon.exe” utilizing new IOCTL and Elo API to demonstrate 
     simultaneous drawing on multiple Elo touch screens.
   • USB (0x26) better rejection for zero bezel frame touch.
   • Send user defined Smartset commands in EloOptions.ini when USB driver loads.
   • Updated Elo logo, icon and user license agreement.

v6.0.0
   • Support Windows XP (32bit with SP3).
   • New calibration approach (no need for HidCal utility, original PreCal implementations removed).
   • Auto mapping touch to display on Win7/8.
   • Provide options for selecting different touch mode.
   • Updated EloPrecal debugging/testing utility.
   • Reduced package size.

v6.1.0
   • Calibration with XY swapped/rotated.
   • MS logo warning on XP during setup. 
   • Reboot after installation/uninstallation is no longer required.
   • Calibration logging feature.
   • 6-Touch IR support.
   • Auto sizing bug fix (wrong increment cycle count).
   • Enable controller's mouse mode on XP.
   • Auto mapping of touch-to-display for Windows 8 and Windows 8.1.
   • Alternative approach for calibration.

v6.2.0

   • USB driver not loaded unless the cable if re-plugged or system is rebooted. 
   • Provide options (EloOptions.ini) to use driver calibration instead of controller calibration. 
   • Correct the pCap firmware version shown in the property page. 
   • Support both new and old firmware for Optical touch monitors. 
   • Provide options to limit number of touches (please see Readme). 
   • IDS improvements: slow response, incorrect initial touch status, incorrect power status report. 

v6.2.1

   • Check the 2521 controller firmware version then apply onboard calibration if it's 6.2 or newer.
   • Need to retrieve controller firmware version from the iProduct field for certain controllers.
   • IDS: set/get monitor power status using Elo VCP codes.

v6.3.0

   • Border touch warning for 2515-07 monitors.
   • Calibration of multiple monitors in spanned display mode.
   • Bug fix where for certain touch monitors (IntelliTouch 2500S / S-Cap 5020), the user is
     continuously being prompted to calibrate their touch monitor(s) after reboot.
   • Bug fix for not mapping touch to display after calibration is performed in Windows 8.1.
   • Bug fix for partially removing Elo files after user confirmed not to proceed with uninstallation.

v6.4.0

   • Mouse mode support on all platforms.
   • Edge acceleration value changes after calibration.
   • Lost touch in ESD test.
   • Touch sensitivity options for 2701, 2521 and 2515-07.
   • Touch visual feedback for calibration testing.
   • Hide mouse curser (system wide).
   • Option to enforce single-touch.
   • EloDriverDefaults.exe (added 2 more parameters)
   • Calibration issue on IDS monitors (resolution not reported correctly, touch targets off position).
   • Support additional IntelliTouch Pro monitors.
   • Adopt new product names IntelliTouch and IntelliTouch Pro.
   • Elo API: Get touch point returns either raw or calibrated points.
   • Missing EloService during silent installation.
   • EloConfig UI shows garbage text in some systems.
   • Calibration on spanned display with rotation.
   • Avoid multi-instance of EloConfig.exe.
   • UI Constraints in CommonSetting Dialog


v6.4.1

   • User's choice for "Single Touch Mode" is not saved between reboots.
   • Touch count was incorrectly limited to 4 in some Optical monitors.
   • Set touch limit did not work correctly for certain pCap.
   • Beep settings and HidCursor did not retain the states between sessions.
   • Support more pCaps.
  • Improve double-click performance.
  • Right-click and hold to bring up context menu.

v6.4.2
  • Fix the occasional setup failure especially with some fresh.
  • Certain IR monitors lost touch after 3-point calibration.

v6.4.3

  • Support 10-touch pCap (PID 0x212C).
  • Support 10-touch IR (PID 0x13).
  • Bug fix for EloDriverDefaults.exe.

v6.4.4 beta

  • Fix "EnableOneTouch" using EloSetup and EloOptions.ini.
  • During setup, it takes too long before the license dialog box shows up.
  • EloDriverDefaults has not been fully tested for this beta release. 


v6.5.0 (04-13-2015 v6.5.0.23)

  • Configure Beep, Touch mode and Enforce single touch as per-device settings.
  • Double-click settings (speed and size).
  • Right-click button (in mouse mode only).
  • Per-monitor touch property settings using EloOptions.ini and EloDriverDefaults. 
  • Support pCap PID 0x67.
  • Setup supports more user defined settings under [Setup Options] in EloOptions.ini.


v6.5.0 b35 (04-29-2015)

  • Incorrect prompt for re-calibration with IR monitors.
  • Fix calibration issue when IRAutoCalibration is enabled on system with IR and pCap.
  • Connected serial touch devices not installed during silent installation.
  • Installation on POSReady 2009 prompting for mouse drivers.


v6.6.0 RC7 (10-20-2015, custom release)

  • Custom touch-to-display mapping for pCap and IR (after install).
  • Right-click button sometimes stuck with the "On" state.
  • Spanned mode setup dialog box shows up unexpected.
  • Prompt for calibration when invoking the Right-click button when the monitor is calibrated.
  • IR calibration data in EloOptions.ini not get applied during calibration.
  • Motherboard beep on Win8.1.
  • Settings defined under [Setup Options] in EloOptions.ini will apply to new devices.
  • EloTouchZones shows blank dialog box with certain system locales.
  • EloWritePRM bug fix.

v6.7.0  (10-02-2015)

  • Supporting more pCaps.
  • API bug fix: EnableTouch, Get/Set Max Touch.
  • EloTouchZones show blank UI for certain system locales.

v6.8.0  (02-29-2016)

  • Support new IntelliTouch controller (PID 0x28).
  • Replaced PID 0x214E with 0x8A6E.
  • Verify NVRam Cal data writing during calibration.
  • Use 0x4E7/0x2410 to replace PIDs 0x9570 and 0x991C.
  • Rotation for one-touch pCap.
  • No longer prompt for calibration at end of Setup.
  • AccuTouch issues: prompt calibration on reboot, failed to calibrate, FW version missing in 32 bit OS.
  • Unexpected prompt for calibration on reboot when a calibrated monitor is connected to a new system.
  • Sometimes during calibration, overlapped dialog boxes were observed.
  • Fix calibration failure on 2500U.
  • On some systems, right-click context manual pops up when resumed from S3/S4 modes.
  • Added ini option AutoInvokeCalibration to enable/disable auto invoking calibration.

v6.8.1  (02-23-2016, custom release)

  • Issues when install as mouse device but previous uninstall did not restore inbox HID mouse state. 

v6.8.2 (05-06-2016)

  • EloConfig property page: sometimes two mouse mode checkboxes can be selected.
  • Support onboard calibration for pid 0x28's emulation mode 2521.
  • Indicate pid 0x28 emulation mode in property page with "(e)".
  • During calibration cursor should not show up.
  • Fix for UTLIRDiag where beep setting back to default at start of the utility.
  • Rotate and calibration issue if installed as mouse device for pid x28 or its 2521 emulation.
  • No longer use Smartset commands for retrieving controller serial numbers.
  • Automatic touch to display mapping for pCap 0x8A6E.
  • During calibration, the "Retry" does not work if mouse click mode is Click-on-Touch.

v6.8.3 build9  (07-12-2016)

  • When serial monitors are installed as mouse device, touch mapped to wrong monitor after
    calibration.
  • Right-click context menu does not pop up reliably on certain pCap monitors.
  • Touch still get registered if quick draw through Elo Touch Zone where touch is disabled.
  • Lock certain EloConfig UI options by using EloOptions.ini entry "LockedConfiguration".
  • Retrieve certain controller's serial numbers from their customized configuration
    blocks (PID 0x212C and 0x8A6E).
  • When Cursor Edge Acceleration is enabled, mouse pointer positon is off from   dragging finger.

v6.8.3 build10  (07-14-2016)

  • Re-built and re-WHQLed.

v6.8.4 (07-21-2016)

  • No reboot needed for serial driver installation.
  • Reading controller (PID 0x212C and 0x8A6E) SNs.
  • Reduce calibration startup time (EloConfig /align).

v6.8.5 (07-25-2016)

  • Fix Elo API for setting beep options.

v6.9.0 (09-14-2016)

  • IR failed beam monitoring.
  • EloDriverDefaults fix for ini’s monitor sections.

v6.9.1 (10-12-2016)

  • Support 20-touch IR monitors (PID: 0x13, size: 55/70 in).

v6.9.2 (11-10-2016)

  • Write controller calibration only during manual calibration.
  • Restore controller calibration parameters after user has canceled a calibration session.
  • Added Monitor S/N as one of the device parameters.
  • Chinese Traditional text is not displayed correctly on Win10 LTSB.
  • Allow user to use MS API GetMessageExtraInfo to distinguish between finger touch and
    physical mouse click. EloOptions.ini has detailed instructions.

v6.9.3 (12-19-2016)

  • Legacy touch monitors in span mode: touch and hold causes shoot-ups.
  • Chinese text too small on some Win10 LTSB systems.
  • Display waiting message before display 1st calibration target.
  • Sometimes need to touch the 1st target multiple times during calibration.
  • EloConfig flashes at system start.
  • Command line calibration: allow user to calibrate a touch screen to specified monitor.
  • EloConfig-AboutBox-Identify Monitors: display Elo Monitor Numbers on all monitors 
    connected to the system. 
  • EloConfig - Property page: Checkbox for "Restore Calibration Default" replaced with a Button
    with additional action: turn controller mode settings to default (onboard calibration is off).
  • Span mode settings not persistent between reboots. 

v6.9.4 (12-28-2016)

  • Uninstallation: remove serial installation only if serial driver has been installed.
  • Uninstallation: no longer copies EloDelMe.bat to C:\ root.

v6.9.5 (01-11-2017)

  • EloTouchZones: Right-click on touch-disabled area still brings up the context manual.
  • EloConfig /align: Add more options to align monitor to primary or the non-primary.
    Please see User manual section 3.2.1 for details.
  • PulseTouch preference parameters defined in EloOptions.ini is not applied after installation. 

v6.9.6 (03-02-2017)

  • Supporting 12-touch pCap (PID 0x240C).

v6.9.7 (05-18-2017)

  • Lost touch on Windows 10 Creator (v1703).
  • Restore the “Border Warning” for 2515.
  • Sync up distributed SDK header files.
  • EloConfig - Property: Enable IR Monitor Beep for Elo legacy IR monitors only.

v6.9.8 (08-28-2017)

  • Missing prompt at end of uninstallation of serial drivers.
  • IR Beam Block Monitoring improvements.
  • XP System with 2 PulseTouch monitors freezes at shutdown.

v6.9.8.4 (08-30-2017)

  • EloDriverDefaults crashes. 

v6.9.9 (09-24-2017)

  • Custom build (detect stuck point and power-cycle the device).
  • Correct HID Report feature ID for certain pCaps.
  • Add new device param to turn off device power settings. 


v6.9.10 (09-27-2017)

  • Correct HID Report feature ID for certain pCaps.
  • Correct the Elo support link in AboutBox.
  • Show PID on EloConfig’s Property Page.

v6.9.11 (Dec. 05 2017)

  •Some touch monitors failed to switch to digitizer mode after wakeup.

v6.9.12 (12-18-2017)

  • Mapping multiple APR Cal file from network storage.
  • Mapping certain pCap touch monitors with monitor serial number stored in NVRAM.
  • No touch after uninstallation. 
  • Fix Elo API EloSetCalData issue with EloWriteCtrlCalData utility.
  • Added version lock for using Elo SDK.

v6.9.14 (02-02-2018)

  • Support more pCaps (0x080B and 0x080C)
  • Security venerability issue in EloService execution path.
  • Fixed hanging issue for APR flash download progress dialog box.

v6.9.15 (02-26-2018)

  • Fix right-click button tool in mouse mode.
  • Calibration session invoked by pressing Enter key after reboot.
  • EloConfig: set focus to the Close button at system start up and each time invoked from desktop.

v6.9.16 (03-16-2018)

  • Add option to generate kernel level logging in Windows Event Log.

v6.9.17 (06-18-2018)

  • EloConfig: show controller model information in the Property page.
  • Add PID 0x28 into touch sensitivity supporting list.
  • Stricter checking for previous installed Elo package during new installation.
  • Kernel mode multi-touch information logging.

v6.9.18 (08-03-2018)

  • USB driver fix for gaps showing when flicking in corner area.
  • USB driver fix (workaround) for drawing line shoot ups.
  • Updated Elo logo.

v6.9.19 (10-17-2018)

  • Hidden Taskbar not shown after rotating the monitor 90 degrees and followed
    by calibration on Windows 7.
  • Elo Serial installation folder remains after uninstallation.
  • EloX crashes
  • USB Controller reset.

v6.9.20 (02-11-2019)

  • Add driver support for the new pCap monitor (PID 0x2902)
  • Fix EloConfig startup error in Windows XP.

v6.9.21 (3-21-2019)

  • Internal only, not released.

v6.9.22 (5-16-2019)

  • EloConfig: new option in EloOptions.in to map touch to Elo monitor.
  • USB driver: driver support for new pCap monitor (7in PID 0x1080).
  • EloSetup: Smartset commands in EloOptions.ini not executed with serial interface.
  • EloCalMgr: v2.5.2, new command line option /setdef to set controller defaults.
  • Use driver calibration for AT Serial interface.
  • Calibration failure on ForceMouse mode with video rotation.
  • Show configuration file version (if available) on pCap PID 0090 in Properties page 


v6.9.23 (08-23-2019)

  • EloConfig: fixed handle leaks.
  • Support pCap PID 0x801 (65in, 40Touch).
  • Support pCap PID 0x2903 (15.6in)

v6.9.24 (12-09-2019)

  • EloOptions.ini: 
      Options to map touch to primary or non-primary. 
      Option to install service reporting.
  • Support pCap PID 0x820 (10Touch).


v7.0.0.42 (07-24-2020)

  • Include Elo Service Reporting installation
  • Updated dll, User manual
  • Provide users options to launch Clean Screen session. This version supports
    systems with only one Elo touch monitor connected.
  • Keyboard shortcut (CTRL+RESET) to reset controller.
  • Support CTR-835600 RS232 Based Controller.
  • Passing Microsoft HLK/HCK Driver Certification for Windows 10/8.1/8/7
  • Support Displaylink PulseTouch and AccuTouch.
  • Added Note on Installation for Windows XP.
  

v7.0.1.4 (08-13-2020)

  • Provide users options to launch Clean Screen session. This version supports systems
    with multi Elo touch monitors connected.
  
v7.0.2.6 (11-12-2020)

  1. USB drivers: Support 2 more touch monitors (PID 0x816 with Active Pen, PID 0x820
     with report 0x17).[WINMT-51].
  2. EloConfig: multiple-touch screen support for Screen Cleaning Notifications.[WINMT-53]
  3. EloConfig: Keyboard controller reset: 3 fast press of CTRL key, no longer use
     Windows Hotkeys. Provided EloOptions.ini option to turn this feature off. [WINMT-61]
  4. EloConfig: Run EloProbe “Common Settings”.[WINMT-46].
  5. EloResetController.exe: Porting controller reset functions from 6.9.12 with additional
     checking of running calibration session.[WINMT-60]
  6. EloDriverDefaults: support turning on/off “LogKernelEvents”. [WINMT-62]
  7. EloCalMgr.exe: added new command line options to retrieve or set controller 
     calibration data:[WINMT-48]
     /get_cal_data: retrieve current controller calibration data and save it in EloCalMgr.ini.
     /set_cal_data: enable controller calibration with calibration data stored in EloCalMgr.ini. 
  8. EloConfig: display PID and HID Report ID in property page's “Controller Model Name” field.

v7.0.3.1 (12-04-2020)

  1. In EloSetup and EloDriverDefaults projects: Copy missing part from v6.9 to add 
     "PCapFrozenTouchRecovery" feature into Registry according to the settings in EloOptions.ini.

v7.1.0.3 (02-04-2021) 

  1. Support PID 0x865 (CTR-835600) [WINMT-50], and PID 0xD22 (CTR-826019) [WINMT-68].
  2. Occasional system BSOD when LogKernelEvents or PCapFrozenTouchRecovery is enabled in
     EloOptions.ini.[WINMT-72].
  3. If touch controller does not support mouse mode and Elo driver is in mouse mode,
     kernel memory will be corrupted when multiple fingers touch the screen. 
     The fix is to allocate proper size of memory.[WINMT-73]
  4. Controller serial number missing in property page for RS232 interface.[WINMT-75]..
  5. ELoConfig: language resource correction for drag delay and untouch timeout page.
  6. Elo SDK manual changed to PDF format.[WINMT-70].
  7. EloProbe: v1.0.56 collect OS SKU information
  8. EloConfig should not respond when F1 key is pressed.[WINMT-66].
  9. EloResetController supports DDC/CI command (EloResetController.exe /ddcci) to
     restart touch controller.

v7.1.1.0 (02-17-2021) 

  1. Prompt users to remove if an existing Elo driver is detected and stops installation.
     If in silent mode, the setup will terminate and returns error (value 1) to the
     calling batch process [WINMT-78]. This is an old bug carried over from MT 6.9.20.
  2. Digital sign EloVideoConfig.dll and Devcon.exe (32/64 bit) [WINMT-81].
  3. Running EloConfig.exe no longer depends on the presence of devcon.exe


v7.2.0.7 (06-01-2021) 

 1. Fixed EloConfig.exe does not run with non-admin account.[WINMT-84]. Current user 
    must log off (sign out) before another user logs in.
 2. Dual monitor mapping swapped after system reboot with USB C cable or 7000L [WINMT-83]
 3. No touch on PID 0x820 Report ID 0x18 [WINMT-86]
 4. EloConfig: Firmware version is not shown correctly for controller PID 0x90 [WINMT-90]
 5. Uninstallation not working on some Windows 7 Embedded systems.
 6. Driver signed with new DigiCert EV certificates.
 7. Driver fixed for PID 2902/2903 to work with new firmware [WINMT-88]
 8. Dynamic ForceMouse through EloDriverDefaults [WINMT-91]
 9. Correct kernel memory pool alocation tags (possbile cause of BSOD).
 
  
v7.2.1.5 (09-13-2021)

 1. Add support for 2 pCaps:
    PID 0x2910 (COF CAB-TP-SCN-COF-85-F-R)
    PID 0x2927 (COF CTR-824022) [WINMT-93]
 2. Add "Enable Drag" option for Click-on-touch (COT) and Click-on-release (COR) [WINMT-99]
 3. Support Push-To-Talk in digitizer mode if COR with "Enable Drag" has been selected. 
 4. EloProbe: collect Elo monitor's SN/PN through VPC.
 5. Elo Service Report Client/Server: collect system local, shorten some reporting parameters.
 6. EloConfig: Touch mode "Mouse emulation" changed to "Normal".
 7. USB Driver: fix touch issue during device enumeration on system with multiple touch 
    monitors [WINMT-92]. 

v8.0.0.10 (02-08-2022)

 1. Supporting HLK for Windows 11 (Win11 SDK/WDK/VS2019).
 2. Include Touch Analyzer as an optional installation [WINMT-47]
 2. USB driver: fix an integer overflow in untouch timeout settings [WINMT-105]
 3. EloConfig: disable touch is not saved [WINMT-110]
 4. Dropped support for Windows XP, support Windows Server 2022.

v9.0.0.23 (02-28-2023)

 1. EloConfig: UI overhaul; major functions are accessible from top-level UI selections [WINMT-132].
 2. Beep Options: Provides more beep sounds [WINMT-130].
 3. Function and UI redesign:
      Touch zone,
      Clean Screen,
      Edge Acceleration.
 4. Software Keyboard: can be invoked anytime regardless if the OS has been configured as tablet or not.
 5. New function to config a single-click to behave as a double-click.
 6. Support more controllers:
      pCap: 80H84 (with serial interface), mouse-mode pCap.
      pCap: 81H84 (with serial interface), single-touch digitizer.
      pCap: with option to switch mouse-mode to single-touch digitizer through OSD.
      IR: PID 0x13 with updated VID.
      pCap pid 0x8A6E: Support controller configured as native mouse [WINMT-139]. 
 7. Improve reliability of controller reset (by Double-Press the CTRL key on a keyboard [WINMT-135]).
 8. User manual and SDK manual: use RTF format instead of PDF [WINMT-134].
 9. EloProbe: allow users to use console output redirection [WINMT-133].
 10. Major bug fixes:
    WINMT-114: Support new VCP code B5 (humidity).
    WINMT-127: Touch monitor (pid 0x7200) did not draw correctly.
    WINMT-128: Simplify Service Reporting Client (remove local logging, network resume).
    WINMT-129: EloConfig: identify AT 2216 and 2218 and show accordingly.
    WINMT-145: ini's Touch sound settings not picked up for newly plugged in devices.
    WINMT-146: Serial installation did not work if hardware handshaking set to 1.
    WINMT-149: EloDriverDefaults: -r option did not work for controller pid 0x8A6E.
    WINMT-154: Unexpected characters in EULA text.
    WINMT-162: Calibration lost after unplug video cable under mouse-mode in  portrait mode.
    WINMT-163: EloResetController: simplify usage options, more meaningful console output. 
    WINMT-170: Simplify ini settings for enabling frozen touch detection.
    WINMT-173: IDS-IR: no touch under "Click on Finger Down".
    WINMT-175: Span mode: touch calibration lost after reboot.

v9.0.1.5 (06-05-2023)

   WINMT-178: Monitor (pid 0x26) lost touch after reboot if Single-touch selected in Touch Settings.
   WINMT-180: EloConfig: Touch settings, sometimes more than one radio buttons got selected.
   WINMT-181: EloSerRptClient not working. 
   WINMT-182: EloConfig: Calibration data not saved on legacy monitors with mouse-mode installation.
   WINMT-184: ELoConfig: After calibration, Elo IR monitor touch got rotated if USB cable re-plugged.
   WINMT-185: Support pCap (0x820) 1099L with serial interface.
   WINMT-186: Support pCap 0x1C00 in mouse-mode (10in).
   WINMT-190: EloConfig: report legacy controller's diagnostic codes.
   
v9.2.0.8 (08-27-2024)
  USB driver: 
    - Add Support for PID 0x1080 with active mouse collection. Add Support for PID 0x1080 
      with Auto-Detect firmware (first implemented in 1304L monitor) [WINMT-210]
    - Add Support for new touch controller VID:PID 0x04E7:0x0843 
      (first implemented in 4304L monitor) [WINMT-207]
    - Add Support for new touch controllers VID:PID 0x2FE9:0x0013 and 0x04E7:0x0013 
      (first implemented in 5053L, 5553L, 6553L, 5054L, 5554L) [WINMT-205]
  RS232 driver: 
    - Fix problem: Setup is hanging when searching for Elo monitor serial port [WINMT-217]





----------- END OF FILE ----------