 Elo XP Universal Driver for Windows 2K/XP and Windows Vista

                      Release 4.6.3b
                      August 23, 2007
                     Elo TouchSystems
         A Division of Tyco Electronics Corporation


Elo Universal Driver contains native 32-bit drivers designed 
for Windows 2K/XP and Windows Vista, a setup program, video alignment 
program, control panel program, tool tray application 
and right button application for Elo TouchSystems' touchmonitors.  

=============================================================

Note: This Driver's User Manual is valid for all XPU 
drivers version 4.X.X


=============================================================
Supported Touchmonitors and Elo Touchscreen Controllers
=============================================================

   - All Elo Entuitive brand touchmonitors with a USB
     controller

   - Elo USB Controllers (IntelliTouch(R) 2216, 2600, 2500U,
     2700, 2701, AccuTouch(R) 3000U, CarrollTouch(R) 4000U, 
     4500U, Surface Capacitive 5000, 5020)

   - All Elo Entuitive brand touchmonitors with an internal
     serial controller

   - Elo Serial Controllers (IntelliTouch(R) 2500S, 2310B, 
     2216, 2310, 2300, 2700, 2701, AccuTouch(R) 2210, 
     CarrollTouch(R), 4000S, 4500S, Surface Capacitive 5000, 5020)

   --------------------------------------------------------
  |                                                        |
  | This driver does not support Elo PC-Bus controllers.   |
  |                                                        |
  | Refer to www.elotouch.com for availability of drivers  |
  | for these products.                                    |
  |                                                        |
   --------------------------------------------------------

================================================================
Installing Elo Universal Driver Windows 2K/XP or Windows Vista
================================================================

Note: you must have administrator access rights on your 
Windows 2K/XP or Windows Vista to install Elo Universial 
Driver for Windows. 

Shutdown your computer and connect your touchmonitor as described
in the accompanying documentation. Restart your computer.

Windows 2K/XP and Windows Vista Installation:
--------------------------------------------

Browse to the directory containing the driver installation 
package files. 

Double click on EloSetup.exe to run the install application.

=================================================================
Uninstalling Elo Universal Driver Windows 2K/XP or Windows Vista
=================================================================

1. After Windows loads, click the Start button, click Settings, 
   and then click Control Panel. 

2. Double-click the Add/Remove Programs icon or Programs and Features (Vista)

3. Select Elo Universal Driver from the list of
   uninstallable programs on the Install/Uninstall tab.

4. Click the Add/Remove or Uninstalled button then follow the directions on
   your screen.

=============
Release Notes
=============

- A touch may not wake the system when in Stand-by power save
  mode. Move the mouse or press a key on the keyboard to return
  from Stand-by mode. Disable Stand-by mode in the Power
  Management control panel to avoid this issue when the USB
  touchscreen is your only input device.

- For Windows Vista users, touch may not wake the system when ANY Energy saving Power Plan 
  is enabled. Move the mouse or press a key on the keyboard to return from Energy saving mode.

- Full Screen DOS sessions are not supported. However, windowed
  DOS mode is fully supported. A touch to a full-screen DOS
  session will cause your system to immediately return to your
  Windows desktop. A mouse can be used to access programs run
  in a Full Screen DOS session.

==============
Contacting Elo
==============

www.elotouch.com

e-mail: eloinfo@elotouch.com

Elo TouchSystems
A Division of Tyco Electronics Corporation
301 Constitution Drive
Menlo Park, CA 94025
USA
Phone: (800) 557-1458
       (650) 361-4700
Fax:   (650) 361-4747

Elo TouchSystems GmbH & Co. KG
Haidgraben 6
D-85521 Ottobrunn
Germany
Phone: +49 (0) 89/60822-0
Fax:   +49 (0) 89/60822-150

Elo TouchSystems, NV
Diestsesteenweg 692
B-3010 Kessel-Lo
Belgium
Phone: +32 (16) 35-2100
Fax:   +32 (16) 35-2101

Copyright (c) 2007 Elo TouchSystems
All rights reserved.

