
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V130.bin ; SA20000QF60V130.bin
  BIOS Checksum : 4575;DDC1
  BIOS String   : 
  Release Date  : 2018/09/11

  Owner         : Paul.Li
  Requester     : 
  Customer      : ELO

  Release Description:
		1.Hidden Serial Port Console Redirection item.	
		2.Release SA20V130 BIOS.	

  Release BIOS Information:
SA20000HI60V130.BIN --- System BIOS and fullsku Me for H81(ME9.1.35.1006)
SA20000QF60V130.BIN --- System BIOS and fullsku Me for Q87(ME9.1.45.3000)

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X037.bin ; SA20000QF60X037.bin
  BIOS Checksum : BF07;F5C6
  BIOS String   : 
  Release Date  : 2018/09/04

  Owner         : Paul.Li
  Requester     : 
  Customer      : ELO

  Release Description:
		1.Modify AMT SOL function fail issue for Q87.		

  Release BIOS Information:
SA20000HI60X037.BIN --- System BIOS and fullsku Me for H81(ME9.1.35.1006)
SA20000QF60X037.BIN --- System BIOS and fullsku Me for Q87(ME9.1.45.3000)

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X036.bin ; SA20000QF60X036.bin
  BIOS Checksum : E54C;F79D 
  BIOS String   : 
  Release Date  : 2018/08/27

  Owner         : Paul.Li
  Requester     : 
  Customer      : ELO

  Release Description:
		1.Update Intel ME RC code to solve ME function fail issue.
		2.Update AMISetupNvLock Module to solve uefi os can not install issue.
		3.Show network stack item.		
		4.Modify temperature unit.
  Release BIOS Information:
SA20000HI60X036.BIN --- System BIOS and fullsku Me for H81(ME9.1.35.1006)
SA20000QF60X036.BIN --- System BIOS and fullsku Me for Q87(ME9.1.45.3000)

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X035.bin ; SA20000QF60X035.bin
  BIOS Checksum : C447;F24A 
  BIOS String   : 
  Release Date  : 2018/08/14

  Owner         : Paul.Li
  Requester     : 
  Customer      : ELO

  Release Description:
	1.Update CPU Microcode to 25 Version.
	2.Update ME firmware to ME91351006/ME91453000.

  Release BIOS Information:
SA20000HI60X035.BIN --- System BIOS and fullsku Me for H81(ME9.1.35.1006)
SA20000QF60X035.BIN --- System BIOS and fullsku Me for Q87(ME9.1.45.3000)

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X034.bin ; SA20000QF60X034.bin
  BIOS Checksum : CB43;78ED 
  BIOS String   : 
  Release Date  : 2018/08/06

  Owner         : Zhijun.Hu
  Requester     : 
  Customer      : ELO

  Release Description:
	1.Add AMISCE Support.
	2.Remove PCIE Hot plug for AMISCE support.


  Release BIOS Information:
SA20000HI60X034.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X034.BIN --- System BIOS and fullsku Me for Q87

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V129.bin ; SA20000QF60V129.bin
  BIOS Checksum : 7022;A1B6
  BIOS String   : 
  Release Date  : 2018/04/13

  Owner         : Wangqing.qiu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
	Release BIOS

  Release BIOS Information:
SA20000HI60V129.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V129.BIN --- System BIOS and fullsku Me for Q87

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X033.bin ; SA20000QF60X033.bin
  BIOS Checksum : AB23; 07E4
  BIOS String   : 
  Release Date  : 2018/04/02

  Owner         : Wangqing.qiu
  Requester     : 
  Customer      : ELO

  Release Description:
SA20X033.a	Auto configure usb BT function.
	
  Release BIOS Information:
SA20000HI60X033.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X033.BIN --- System BIOS and fullsku Me for Q87

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X032.bin ; SA20000QF60X032.bin
  BIOS Checksum : 103C;  05B7
  BIOS String   : 
  Release Date  : 2018/02/27

  Owner         : Wangqing.qiu
  Requester     : 
  Customer      : ELO

  Release Description:
SA20X032.a	Rebuild BIOS binary to show temperature unit accurately.

  Release BIOS Information:
SA20000HI60X032.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X032.BIN --- System BIOS and fullsku Me for Q87

//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X031.bin ; SA20000QF60X031.bin
  BIOS Checksum : 1FFD;  5A85
  BIOS String   : 
  Release Date  : 2018/02/27

  Owner         : Wangqing.qiu
  Requester     : 
  Customer      : ELO

  Release Description:
SA20X031.a	Update Microcode to M32306C3_00000024

  Release BIOS Information:
SA20000HI60X031.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X031.BIN --- System BIOS and fullsku Me for Q87
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V128.bin ; SA20000QF60V128.bin
  BIOS Checksum : 8EE5;3DF4 
  BIOS String   : 
  Release Date  : 2017/12/18

  Owner         : Wangqing.qiu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
	Release BIOS

  Release BIOS Information:
SA20000HI60V128.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V128.BIN --- System BIOS and fullsku Me for Q87

//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X030.bin ; SA20000QF60X030.bin
  BIOS Checksum : 09E6; 7492
  BIOS String   : 
  Release Date  : 2017/12/12

  Owner         : Wangqing.qiu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X030.a	Tune display of temperature unit.

  Release BIOS Information:
SA20000HI60X030.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X030.BIN --- System BIOS and fullsku Me for Q87
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X029.bin ; SA20000QF60X029.bin
  BIOS Checksum : E8A2; 25BA
  BIOS String   : 
  Release Date  : 2017/11/24

  Owner         : Wangqing.qiu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X029.a	Modify new touch info.

  Release BIOS Information:
SA20000HI60X029.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X029.BIN --- System BIOS and fullsku Me for Q87



//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V127.bin ; SA20000QF60V127.bin
  BIOS Checksum : 8382 ; 8FC5
  BIOS String   : 
  Release Date  : 2017/2/10

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V127.a	Fixed: The PXE cannot use legacy boot

  Release BIOS Information:
SA20000HI60V127.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V127.BIN --- System BIOS and fullsku Me for Q87



//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X028.bin ; SA20000QF60X028.bin
  BIOS Checksum : 47C3; CF88
  BIOS String   : 
  Release Date  : 2017/2/7

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V127.a	Fixed: The PXE cannot use legacy boot

  Release BIOS Information:
SA20000HI60X028.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X028.BIN --- System BIOS and fullsku Me for Q87



//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V126.bin ; SA20000QF60V126.bin
  BIOS Checksum : 524A; 58E2
  BIOS String   : 
  Release Date  : 2017/1/17

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V126.b	Customer request:Modify new touch info.

SA20V126.a	The PXE ROM select the uefi or legacy, Video ROM used the same.

  Release BIOS Information:
SA20000HI60V126.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V126.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V125.bin ; SA20000QF60V125.bin
  BIOS Checksum : 62E2; 16D3
  BIOS String   : 
  Release Date  : 2017/1/3

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V125.a	The CSM control the PXE boot from uefi or legacy

  Release BIOS Information:
SA20000HI60V125.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V125.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V124.bin ; SA20000QF60V124.bin
  BIOS Checksum : 9179; 247E
  BIOS String   : 
  Release Date  : 2016/11/16

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V124.a	Fixed:CSM Boot option filter for UEFI

  Release BIOS Information:
SA20000HI60V124.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V124.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V123.bin ; SA20000QF60V123.bin
  BIOS Checksum : 5C8F; 3166
  BIOS String   : 
  Release Date  : 2016/10/13

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20V123.a	Hidden the Intel uefi Lan in setup menu
		Note:Get the TSE source, and modify by EIP170262 

SA20V123.a	Sync. the uEFI & Legacy PXE boot 

  Release BIOS Information:
SA20000HI60V123.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V123.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V122.bin ; SA20000QF60V122.bin
  BIOS Checksum : 988C; 01E8
  BIOS String   : 
  Release Date  : 2016/9/21

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
Rebuild for BIOS Version sync.
And formal release BIOS V122

  Release BIOS Information:
SA20000HI60V122.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V122.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V121.bin ; SA20000QF60V121.bin
  BIOS Checksum : 99E2 ; EBC5
  BIOS String   : 
  Release Date  : 2016/9/20

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
Formal release BIOS V121

  Release BIOS Information:
SA20000HI60V121.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V121.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X027.bin ; SA20000QF60X027.bin
  BIOS Checksum : 94A2; 8E78
  BIOS String   : 
  Release Date  : 2016/9/9

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X027.b	Open the CSM parameters for UEFI PXE boot.
		Note:If the boot mode are not match(UEFI/Legacy), system is blakc screen. 

SA20X027.a	Update the UEfiNetworkStack module for UEFI IPV6 PXE Boot.

  Release BIOS Information:
SA20000HI60X027.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X027.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V120.bin ; SA20000QF60V120.bin
  BIOS Checksum : 42A1 ; 287B
  BIOS String   : 
  Release Date  : 2016/8/31

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X026.a	Customer request: Clear CMOS, reset the BIOS password.

  Release BIOS Information:
SA20000HI60V120.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V120.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V119.bin ; SA20000QF60V119.bin
  BIOS Checksum : 32F8 ; 1C4D
  BIOS String   : 
  Release Date  : 2016/7/4

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X025.a	Modify the Setup menu for ELO's behavior.

  Release BIOS Information:
SA20000HI60V119.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V119.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X025.bin ; SA20000QF60X025.bin
  BIOS Checksum : 15ED ; 7EC5
  BIOS String   : 
  Release Date  : 2016/6/24

  Owner         : thomas.lu
  Requester     : 15ED ; 7EC5
  Customer      : ELO

  Release Description:
SA20X025.a	Modify the Setup menu for ELO's behavior.

  Release BIOS Information:
SA20000HI60X025.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X024.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X024.bin ; SA20000QF60X024.bin
  BIOS Checksum : 6E2B ; 925E
  BIOS String   : 
  Release Date  : 2016/5/11

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X024.a	Modify the Setup menu for ELO's behavior.

  Release BIOS Information:
SA20000HI60X024.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X024.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X023.bin ; SA20000QF60X023.bin
  BIOS Checksum : 9D00 ; 43E1
  BIOS String   : 
  Release Date  : 2016/4/14

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X023.c	Support the Default password and customer setup flow

SA20X023.b	If system does not Boot device, show the error message and hold.

SA20X023.a	Support the UEFI PXE Boot

  Release BIOS Information:
SA20000HI60X023.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X023.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X022.bin ; SA20000QF60X022.bin
  BIOS Checksum : 0C82 ; 2429
  BIOS String   : 
  Release Date  : 2016/3/21

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X022.a	Fixed: The Efi boot does not control the Com3,4,5
		Note: Reference the SA20X009.c SA20X009.d

  Release BIOS Information:
SA20000HI60X022.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X022.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V118.bin ; SA20000QF60V118.bin
  BIOS Checksum : 65CB ; 1593
  BIOS String   : 
  Release Date  : 2016/3/9

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X021.b	Hidden the RAID mode for H81

SA20X021.a	Customer request:Add new touch info 0x03EB8A6E

  Release BIOS Information:
SA20000HI60V118.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V118.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X020.bin ; SA20000QF60X020.bin
  BIOS Checksum : E289 ; 9EE8
  BIOS String   : 
  Release Date  : 2016/2/24

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X020.a	Fixed: RTC fail with SA20X019.a

  Release BIOS Information:
SA20000HI60X020.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X020.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X019.bin ; SA20000QF60X019.bin
  BIOS Checksum : 1425 ; EF5E
  BIOS String   : 
  Release Date  : 2016/2/23

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X019.a	Workaround: Reset for USE device init

  Release BIOS Information:
SA20000HI60X019.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X019.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X018.bin ; SA20000QF60X018.bin
  BIOS Checksum : 1A41 ; 1DA3
  BIOS String   : 
  Release Date  : 2016/2/18

  Owner         : thomas.lu
  Requester     : Vincent.Lai
  Customer      : ELO

  Release Description:
SA20X018.a	Switch Boot Option ODD, UEFI, HDD, USB,NETWORK

  Release BIOS Information:
SA20000HI60X018.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X018.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V117.bin ; SA20000QF60V117.bin
  BIOS Checksum : 3DBD ; AE2A
  BIOS String   : 
  Release Date  : 2016/1/28

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X017.a	Open the UEFI Boot Items

  Release BIOS Information:
SA20000HI60V117.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V117.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V116.bin ; SA20000QF60V116.bin
  BIOS Checksum : 9D33 ; 8103
  BIOS String   : 
  Release Date  : 2016/1/7

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X016.a	Fixed:The the Touch info cannot display, when USB devices plug-in some port.

  Release BIOS Information:
SA20000HI60V116.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V116.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V115.bin ; SA20000QF60V115.bin
  BIOS Checksum : 533B ; 07BB
  BIOS String   : 
  Release Date  : 2015/12/7

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X015.d	Set the USB transfer time-out from 20 sec to 1 sec

SA20X015.c	Updatge the Touch info String of 0x04E70020 to: "CTR-270100-IT-RSU-00R"

SA20X015.b	Change the F5/F6 to CTRL+F5/F6 for Com5 and EDID program

SA20X015.a	The the Touch info for only one usb port.

  Release BIOS Information:
SA20000HI60V115.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V115.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : ntel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V114.bin ; SA20000QF60V114.bin
  BIOS Checksum : 4930 ; DE42
  BIOS String   : 
  Release Date  : 2015/8/12

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20V114.b	Customer request:Add new touch info from 0x04E72007 to x04E72100

SA20V114.a	Disabled the USB S4 wakeup 

  Release BIOS Information:
SA20000HI60V114.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V114.BIN --- System BIOS and fullsku Me for Q87



//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : ntel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60V113.bin ; SA20000QF60V113.bin
  BIOS Checksum : 7774 ; 14C3
  BIOS String   : 
  Release Date  : 2015/8/12

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20V113.a	Customer request:Modify the check ID:0x04E700C0 to 0x04E72007

  Release BIOS Information:
SA20000HI60V113.BIN --- System BIOS and fullsku Me for H81
SA20000QF60V113.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X014.bin ; SA20000QF60X014.bin
  BIOS Checksum : CCFE; 0FBC
  BIOS String   : (SA20000ss60X014) EVALUATION ROM FOR sssV1.11-NOT FOR SALE
  Release Date  : 2015/2/26

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X014.c	For official release, BIOS setup shows V Version.
		Customer request: Project Version & Sign On message show the SKU(H81/Q87)
		There are two solution:
		1. Set "OFFICIAL_RELEASE" = 1 to recompiler.
		2. Modify the Sign on Message by BCP Tool.
			Format:	"**** DMS-SA20 BIOS sssV1.xx (xx/xx/xxxx) ****"
			sss should be H81 or Q87

SA20X014.b	Update the Touch for goes into setup

SA20X014.a	Customer request:Modify Touch info

  Release BIOS Information:
SA20000HI60X014.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X014.BIN --- System BIOS and fullsku Me for Q87


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X013.bin ; SA20000QF60X013.bin
  BIOS Checksum : 87AD ; F0E7
  BIOS String   : 
  Release Date  : 2015/1/27

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X013.b	Update Logo to 1024*768

SA20X013.a	For official release, BIOS setup shows V Version.

  Release BIOS Information:
SA20000HI60X013.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X013.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X012.bin ; SA20000QF60X012.bin
  BIOS Checksum : 59D0; A237
  BIOS String   : 
  Release Date  : 2015/1/26

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X012.f	Change the Customer Logo

SA20X012.g	Customer request: Show BIOS name : SA20H81X0__ & SA20Q87X0__

SA20X012.f	EE request: disabled USB Beep

SA20X012.e	Add SYSTEM_MANUFACTURE & CHASSIS_MANUFACTURE in setup menu

SA20X012.d	Update the Moude & Softkey module

SA20X012.c	Show the touch Info

SA20X012.b	Workaround: The USB device boot fail.

SA20X012.a	Fixed: the resulation is changed, when SATA mode to Raid mode.

  Release BIOS Information:
SA20000HI60X012.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X012.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X011.bin ; SA20000QF60X011.bin
  BIOS Checksum : B03C; 716A
  BIOS String   : 
  Release Date  : 2014/12/18

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X011.b	Add SLP module for OA2.1

SA20X011.a	Modify the MOuse point

  Release BIOS Information:
SA20000HI60X011.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X011.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X010.bin ; SA20000QF60X010.bin
  BIOS Checksum : 3A99; 8318
  BIOS String   : 
  Release Date  : 2014/12/16

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X010.a	Set the default value of Cash Drawer Voltage to 24V

  Release BIOS Information:
SA20000HI60X010.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X010.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X009.bin ; SA20000QF60X009.bin
  BIOS Checksum : EBA9; EB76
  BIOS String   : 
  Release Date  : 2014/12/12

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X009.g	Update Thermal Policy

SA20X009.f	Set default enabled TPM for Q87

SA20X009.e	Update the System Product Name to "Elo AiO"

SA20X009.d	Support Com3,4 Board

SA20X009.c	Support F5/F6 for Com5 and EDID program

SA20X009.b	Correct the Fix boot order

SA20X009.a	Support Keyboard mouse


  Release BIOS Information:
SA20000HI60X009.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X009.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X008.bin ; SA20000QF60X008.bin
  BIOS Checksum : AC75; 188A
  BIOS String   : 
  Release Date  : 2014/11/18

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X008.f	EE request: Hidden some CPU item.

SA20X008.e	Customer request: Set DEFAULT_QUIET_BOOT enabled

SA20X008.d	Init PECI for S3

SA20X008.c	Remove the SIO Deep S5

SA20X008.b	Support the Watch Dog function

SA20X008.a	Disable the DXE_NO_CON_IN Beep

  Release BIOS Information:
SA20000HI60X008.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X008.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X007.bin ; SA20000QF60X007.bin
  BIOS Checksum : B8FE; 7525
  BIOS String   : 
  Release Date  : 2014/10/14

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X007.d	Correct the PCIe for Project

SA20X007.c	Update the PXE rom & Gbe FW

SA20X007.b	EE request: open the Serial port2, and set to COM5

SA20X007.a	Update thermal Policy

  Release BIOS Information:
SA20000HI60X007.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X007.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X006.bin ; SA20000QF60X006.bin
  BIOS Checksum : F76F; 7FCD
  BIOS String   : (SA20000HI60X006) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/8/25

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X006.o	Update Logo

SA20X006.n	Fixed: Show Memory information during post

SA20X006.m	Modify the debug port for SA-20

SA20X006.l	EE: Modify the USB2 Length

SA20X006.k	Support LAN MAC in serup Main page 

SA20X006.j	Add DMI: Product Name, Serial Number and UUID in serup Main page

SA20X006.i	Add CPU info in serup Main page

SA20X006.h	Create the Smart Fan IV item for CPU Fan

SA20X006.g	Set the SIO GPIO 43,44 item

SA20X006.h	Modify the LED with SUS_LED & GP47 of SuperIO
		Note:The S1 resume callback is called before goes into S1.

SA20X006.g	Add info Report

SA20X006.f	Fixed Lan PXE cannot disabled

SA20X006.e	Modify Logo screen for inforeport

SA20X006.d	EE:Set  PCH 36,37 output to Low

SA20X006.c	Update VBIOS for CTR EDID

SA20X006.b	Set Popup Menu to F11

SA20X006.a	Set Audio SSIDSVID: 13FEBC05.
		OEMEM\COREMOD\4654\CRB\CRBLib.c 

  Release BIOS Information:
SA20000HI60X006.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X006.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X005.bin ; SA20000QF60X005.bin
  BIOS Checksum : E0FA; 82B0
  BIOS String   : (SA20000HI60X005) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/7/25

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X005.e	EE request: set GPIO of PCH 1,36,37 to high 

SA20X005.d	Support GPIO36 & deep S5 control for SuperIO NCT6106D

SA20X005.c	Modify the BIOS string for SA20

SA20X005.b	Remove upsupport module
		
SA20X005.a	Update thermal Policy

  Release BIOS Information:
SA20000HI60X005.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X005.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X004.bin ; SA20000QF60X004.bin
  BIOS Checksum : EF80; 9D5
  BIOS String   : (SA20000HI60X004) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/7/10

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X004.b	Modify the FAN policy

SA20X004.a	Open the BIOS security Options for FPT utility

  Release BIOS Information:
SA20000HI60X004.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X004.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X003.bin ; SA20000QF60X003.bin
  BIOS Checksum : A82C; 361D
  BIOS String   : (SA20000HI60X003) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/7/8

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X003.c	Modify the Fan Speed CruiseTM Mode.
		1 unit is 50PRM

SA20X003.b	Set GPIO36 of SIO is high

SA20X003.a	Set the LED for S0~S5

  Release BIOS Information:
SA20000HI60X003.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X003.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X002.bin ; SA20000QF60X002.bin
  BIOS Checksum : BA66; F8DF
  BIOS String   : (SA20000HI60X002) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/6/27

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
SA20X002.g	HW monitor setting and remove the System Fan.

SA20X002.f	Redefine the SuperIO com port setting:
		Disable the COM 0, 1, and set the default setting: 
			Com C->A, Com D->B, Com E->C, Com F->D

SA20X002.e	Remove not support function

SA20X002.d	Support Q87 & H81 build

		Add Fixed Boot Order

SA20X002.c	Update the Verb Table

SA20X002.b	Remove the AT support

SA20X002.a	Update the VBIOS for DMS-SA20

		Base on the AIMB_274 x046, create the DMS-SA20 project.


  Release BIOS Information:
SA20000HI60X002.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X002.BIN --- System BIOS and fullsku Me for Q87


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : SA20000HI60X001.bin ; SA20000QF60X001.bin
  BIOS Checksum : 1922 ; EE3A
  BIOS String   : (SA20X001) EVALUATION ROM FOR V1.10-NOT FOR SALE
  Release Date  : 2014/6/18

  Owner         : thomas.lu
  Requester     : Winston.Hong
  Customer      : ELO

  Release Description:
Base on the DAC-BJ08 x006, create the DMS-SA20 project.

  Release BIOS Information:
SA20000HI60X001.BIN --- System BIOS and fullsku Me for H81
SA20000QF60X001.BIN --- System BIOS and fullsku Me for Q87



//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : DMS-SA20 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint H81/Q87
    ClockGEN    : Intel ICC
    SuperI/O    : NCT6106D
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X046.bin ; A274X046.rom
  BIOS Checksum : A680 ; 2310
  BIOS String   : (A274X046) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/5/19

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X046.a Fixed AMT console redirection to DOS function fail (Bug ID:0215008)

  Release BIOS Information:
    A274X046.BIN --- System BIOS and fullsku Me.
    A274X046.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X045.bin ; A274X045.rom
  BIOS Checksum : ED13 ; 69A3
  BIOS String   : (A274X045) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/5/14

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X045.a Fixed caseopen function fail after remove AC power. (Bug ID:0215007)
    X045.b Fixed raid card compatibility issue.
    X045.c Add SPI W25Q128FV Vscc table ID.

  Release BIOS Information:
    A274X045.BIN --- System BIOS and fullsku Me.
    A274X045.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X044.bin ; A274X044.rom
  BIOS Checksum : 0xA876 ; 0x18DC
  BIOS String   : (A274X044) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/3/20

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X044.a      Update code base to X035 and ME to 9.0.30.1482.

  Release BIOS Information:
    A274X044.BIN --- System BIOS and fullsku Me.
    A274X044.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X043.bin ; A274X043.rom
  BIOS Checksum : 0x00A5 ; 0x5916
  BIOS String   : (A274X043) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/2/18

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X043.a      Update verb table.

  Release BIOS Information:
    A274X043.BIN --- System BIOS and fullsku Me.
    A274X043.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X042.bin ; A274X042.rom
  BIOS Checksum : 0x3FD1 ; 0x9842
  BIOS String   : (A274X042) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/1/23

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X042.a      Update verb table.

  Release BIOS Information:
    A274X042.BIN --- System BIOS and fullsku Me.
    A274X042.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X041.bin ; A274X041.rom
  BIOS Checksum : 0x0A25 ; 0x6296
  BIOS String   : (A274X041) EVALUATION FOR V1.12 - NOT FOR SALE
  Release Date  : 2014/1/16

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X041.a      Switch audio verb table depends on GPIO 15 and 32.

  Release BIOS Information:
    A274X041.BIN --- System BIOS and fullsku Me.
    A274X041.ROM --- System BIOS.


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : AIMB-274  
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint
    ClockGEN    : Intel ICC
    SuperI/O    : ITE8518E
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274V111.bin
  BIOS Checksum : B8D3
  BIOS String   : **** AIMB-274 BIOS V1.11 (11/26/2013) ****
  Release Date  : 2013/11/26

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X040.b Set display port to be eDP signal for Chrontel 7511 abnormal issue. Also need to update Chrontel firmware.

  Release BIOS Information:
    A274V111.BIN --- System BIOS and fullsku ME.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X040.bin ; A274X040.rom
  BIOS Checksum : FEA4 ; 5715
  BIOS String   : (A274X040) EVALUATION FOR V1.11 - NOT FOR SALE
  Release Date  : 2013/11/20

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X040.b Set display port to be eDP signal for Chrontel 7511 abnormal issue. Also need to update Chrontel firmware.

  Release BIOS Information:
    A274X040.BIN --- System BIOS and fullsku ME.
    A274X040.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X039.bin ; A274X039.rom
  BIOS Checksum : A2F4 ; FB65
  BIOS String   : (A274X039) EVALUATION FOR V1.11 - NOT FOR SALE
  Release Date  : 2013/11/12

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X039.a Fixed some USB ports do not have eject icon in OS with plugging USB device.
    X039.b Fixed USB port cannot detect devices after resume from S4 if you do not plug any USB device when enter S4 state.(Bug ID:000047448)
    X039.c Add PCH check function.

  Release BIOS Information:
    A274X039.BIN --- System BIOS and fullsku Me.
    A274X039.ROM --- System BIOS.


//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//Previous History
//---------------------------------------------------------------------------
//---------------------------------------------------------------------------
//
//   Copyright (c) 2010-2013 Advantech Co., Ltd.
//   This program contains proprietary and confidential information.
//   All rights reserved except as may be permitted by prior written consent.
//
//----------------------------------------------------------------------------
//  Project Name : AIMB-274 
//----------------------------------------------------------------------------
//  Hardware Configuration
//----------------------------------------------------------------------------
    CPU         : Intel Haswell
    Chipset     : Intel LynxPoint
    ClockGEN    : Intel ICC
    SuperI/O    : ITE8518E
    Flash ROM   : Winbond W25Q128FV
//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274V110.bin
  BIOS Checksum : FB7E
  BIOS String   : **** AIMB-274 BIOS V1.10 (08/09/2013) ****
  Release Date  : 2013/8/9

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X038.a Modify VBIOS to fix DP from port C cannot display.

  Release BIOS Information:
    A274V110.BIN --- System BIOS and fullsku Me.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X038.bin ; A274X038.rom
  BIOS Checksum : E38A ; 3BFB
  BIOS String   : (A274X038) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/8/8

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X038.a Modify VBIOS to fix DP from port C cannot display.

  Release BIOS Information:
    A274X038.BIN --- System BIOS and fullsku Me.
    A274X038.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X037.bin ; A274X037.rom
  BIOS Checksum : 0x53A4 ; 0xAC15
  BIOS String   : (A274X037) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/8/7

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X037.a   Remove unused SATA/LAN/MiniPCIe items for L SKU.
    X037.b   Modify setup menu.
    X037.c   Patch 9650SE can't work.

  Release BIOS Information:
    A274X037.BIN --- System BIOS and fullsku Me.
    A274X037.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X036.bin ; A274X036.rom
  BIOS Checksum : 0x3B90 ; 0x9401
  BIOS String   : (A274X036) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/7/30

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X036.a  Update VBIOS to 2173.
    X036.b  System will hang up when pressing num lock or caps lock in setup menu, it has been fixed. 
    X036.c  Revise "X031.f".
    X036.d  Fixed system with AC power and then short CMOS jumper, BIOS date and time will be cleared. 
    X036.e  Improve beep sound of abnormal when XHCI mode is enabled.
    X036.f  Remove PCIE Wake From DeepSx item.

  Release BIOS Information:
    A274X036.BIN --- System BIOS and fullsku Me.
    A274X036.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X035.bin ; A274X035.rom
  BIOS Checksum : D12F ; 29A2
  BIOS String   : (A274X035) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/7/18

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X035.a Fixed system cannot enter IDE mode OS after remote reboot by AMT.(Bug ID:000044955)
    X035.b Fixed Display Port 2 does not have audio output.(Bug ID:000045165)
    X035.c Fix system hang in BIOS Setup random when using PS/2 keyboard.
    X035.d Support AIMB-274 L SKU and remove unused display items.

  Release BIOS Information:
    A274X035.BIN --- System BIOS and fullsku Me.
    A274X035.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X034.bin ; A274X034.rom
  BIOS Checksum : 5C28 ; B49B
  BIOS String   : (A274X034) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/7/3

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X034.a Updated codebase to Aptio 4.6.5.4_VEB_1AQQW027 and ME version to "9.0.13.1402".

  Release BIOS Information:
    A274X034.BIN --- System BIOS and fullsku Me.
    A274X034.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X033.bin ; A274X033.rom
  BIOS Checksum : 2390 ; CF76
  BIOS String   : (A274X033) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/6/13

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X033.a Updated codebase to Aptio 4.6.5.4_VEB_1AQQW026 and ME version to "9.0.10.1372".

  Release BIOS Information:
    A274X033.BIN --- System BIOS and fullsku Me.
    A274X033.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X032.bin ; A274X032.rom
  BIOS Checksum : 8E7D ; 3489
  BIOS String   : (A274X032) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/6/7

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X032.a Default disable "PEG0 - ASPM".(Bug ID:000043497/000043498/000043501)
    X032.b Hide "Setup Item Hidden" item.
    X032.c Enhance PCI Express RAID Card compatibility.

  Release BIOS Information:
    A274X032.BIN --- System BIOS and fullsku Me.
    A274X032.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X031.bin ; A274X031.rom
  BIOS Checksum : CFC7 ; 75D3
  BIOS String   : (A274X031) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/5/23

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X031.a Add second VBIOS to support pure HDMI function.(Bug ID:000041413)
    X031.b Enable spread spectrum of displayport.
    X031.c Modify PCIE wake item string in .SD file.
    X031.d Updated codebase to Aptio 4.6.5.4_VEB_1AQQW025 and ME version to "9.0.3.1347".
    X031.e Fix the issue that SHIFT key of PS/2 keyboard can work at first time only.
    X031.f Fixed system show "Entering MEBX setup menu ......" repeat when press Ctrl+P with some keyboard.
    X031.g Open "GP27 Wake From DeepSx" and "PCIE Wake From DeepSx" items.

  Release BIOS Information:
    A274X031.BIN --- System BIOS and fullsku Me.
    A274X031.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X030.bin ; A274X030.rom
  BIOS Checksum : 0x9868 ; 0x9240
  BIOS String   : (A274X030) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/5/15

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X030.a Revise H/W monitor function.
    X030.b Support ACPI shutdown temperature. 
    X030.c Hide ACPI shutdown temperature item.

  Release BIOS Information:
    A274X030.BIN --- System BIOS and fullsku Me.
    A274X030.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X029.bin ; A274X029.rom
  BIOS Checksum : A9FE ; A3D6
  BIOS String   : (A274X029) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/5/6

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X029.a Update code base to "X024".

  Release BIOS Information:
    A274X029.BIN --- System BIOS and fullsku Me.
    A274X029.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X028.bin ; A274X028.rom
  BIOS Checksum : A435 ; 9E0D
  BIOS String   : (A274X028) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/5/2

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X028.a Disabled all of "PME SCI" from PCIe root port.
    X028.b Enable "Hot Plug" of PCIe root port 0 to fix mini-PCIe devices cannot work if enable "PCIE Root Port Function Swapping".(Bug ID:000043504)
    X028.c Enhance PCI Express RAID Card compatibility.(Bug ID:000043497/000043498/000043501)
    X028.d Fixed password will be clean while RTC_RST# active.

  Release BIOS Information:
    A274X028.BIN --- System BIOS and fullsku Me.
    A274X028.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X027.bin ; A274X027.rom
  BIOS Checksum : 6FFD ; 69D5
  BIOS String   : (A274X027) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/4/25

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X027.a Default disable "PME SCI" of PCIe port 6 to fixed system cannot enter OS after LAN2 wake up from S3/S4/S5.(Bug ID:000043746)

  Release BIOS Information:
    A274X027.BIN --- System BIOS and fullsku Me.
    A274X027.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X026.bin ; A274X026.rom
  BIOS Checksum : 64F0 ; 5EC8
  BIOS String   : (A274X026) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/4/18

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X026.a Fixed X025.e code error.
    X026.b Update code base to "X023"
    X026.c Fixed eDP cannot display if you do not select "VBIOS Default".(Bug ID:000043149)
    X026.d Update VBIOS to version "2170".
    X026.e Remove "PEG1" and "PEG2" items in NB PCIe Configuration.
    X026.f Enhance PCIE RAID Card (adapter 5405 / Highpoint 3510) compatibility on NB PCIe x16 slot.

  Release BIOS Information:
    A274X026.BIN --- System BIOS and fullsku Me.
    A274X026.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X025.bin ; A274X025.rom
  BIOS Checksum : F5D3 ; EFAB
  BIOS String   : (A274X025) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/4/11

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X025.a Modify VBIOS to fixed DP1 cannot display during post.(Bug ID:000043148)
    X025.b Fixed system will auto wake up when enter S1/S3/S4 mode.(Bug ID:000043296)
    X025.c Fixed USB keyboard can wake up system from S4 if you enter S3 first in X86 OS.(Bug ID:000042981)
    X025.d Modify display item string from "LVDS" to "eDP-LVDS".
    X025.e Hide "External SATA" item of normal SATA ports.

  Release BIOS Information:
    A274X025.BIN --- System BIOS and fullsku Me.
    A274X025.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X024.bin ; A274X024.rom
  BIOS Checksum : 2503 ; 1EDB
  BIOS String   : (A274X024) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/4/3

  Owner         : letien.cheng
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X024.a Fixed that mini PCIe Slot.1 (full size) can't detect mini PCIe WIFI card. (Bug #0043049)
    X024.b Change "PCIE Root Port Function Swapping" item value to "Enable" as default.
    X024.c Modify setup info.
    X024.d Modify VBIOS for SI testing.
    X024.e Fixed screen has garbage if enter shell.
    X024.f Program some registers to reduce the boot time of first AT mode boot.
    X024.g Set "DeepSx Power Policies" item value to "Disable" when AT mode.
    X024.h Update code base to "X022a" and ME to "9.0.2.1345"

  Release BIOS Information:
         A274X023.BIN --- System BIOS and fullsku Me.
         A274X023.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X023.bin ; A274X023.rom
  BIOS Checksum : ABBD ; EFFF
  BIOS String   : (A274X023) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/3/27

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X023.a Remove "ECC Support" item in memory configuration.(Bug ID:000042989)
    X023.b Default set SATA to be "AHCI" mode and hotplug and external SATA function default enabled of eSATA port.(Bug ID:000042988)
    X023.c Remove exclamation mark from BIOS signon message.
    X023.d Modify CG mode default order to adjust the resolution during post.

  Release BIOS Information:
    A274X023.BIN --- System BIOS and fullsku Me.
    A274X023.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X022.bin ; A274X022.rom
  BIOS Checksum : F4B8 ; 38FA
  BIOS String   : (A274X022) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/3/15

  Owner         : allenkl.liu
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    X022.a Modify VBIOS to set "Select HDMI level shifter configuration" of EFP2 to be "800mV 2.0dB".

  Release BIOS Information:
    A274X022.BIN --- System BIOS and fullsku Me.
    A274X022.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X021.bin ; A274X021.rom
  BIOS Checksum : 0x7F06 ; 0x03A8
  BIOS String   : (A274X021) EVALUATION FOR V1.10 - NOT FOR SALE
  Release Date  : 2013/3/14

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Updated VBIOS to hsw_2166.
    b. Added to support i211 LAN PXE Option rom.
    c. Added to control RS422/RS485 Termination resistors.
    d. Added eDP and LVDS select item.
    e. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW021.

  Release BIOS Information:
    A274X021.BIN --- System BIOS and fullsku Me.
    A274X021.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X020.bin ; A274X020.rom
  BIOS Checksum : 0xBD4A ; 0xBB25
  BIOS String   : (A274X020.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/2/26

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW020.
    b. Updated VBIOS Setting.

  Release BIOS Information:
    A274X020.BIN --- System BIOS and fullsku Me.
    A274X020.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X019.bin ; A274X019.rom
  BIOS Checksum : 0x7DED ;  0x7BC8
  BIOS String   : (A274X019.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/2/19

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Added to support AT/ATX mode.

  Release BIOS Information:
    A274X019.BIN --- System BIOS and fullsku Me.
    A274X019.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X018.bin ; A274X018.rom
  BIOS Checksum : 0x536C ; 0x5147
  BIOS String   : (A274X018.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/2/5

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Change DeepSx support from EC to PCH.
    b. Updated VBIOS to version 2164.
    c. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW019.

  Release BIOS Information:
    A274X018.BIN --- System BIOS and fullsku Me.
    A274X018.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X017.bin ; A274X017.rom
  BIOS Checksum : 0x1DED ; 0x1BC8
  BIOS String   : (A274X017.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/31

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Added to report sleep status to EC RAM 0x9F.
    b. Fixed system auto wakeup after WOL from S1 by INTEL I217(GbE).
    c. Change "Serial IRQ Mode" item value to "Continuous" as default.    
    d. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW019(Bate).

  Release BIOS Information:
    A274X017.BIN --- System BIOS and fullsku Me.
    A274X017.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X016.bin ; A274X016.rom
  BIOS Checksum : 0xA565 ; 0x0C72
  BIOS String   : (A274X016.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/22

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Modify VBIOS setting.
    b. Modify HD Audio SVID abd SSID to 0x274013FE.
    c. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW018.    

  Release BIOS Information:
    A274X016.BIN --- System BIOS and fullsku Me.
    A274X016.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X015.bin ; A274X015.rom
  BIOS Checksum : 0xDF87 ; 0x7187
  BIOS String   : (A274X015.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/17

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Added to Inform EC for system resume from S1.
    b. Added to support Resume on RI# in DOS mode.
    c. Fixed typo issue for HW monitor information.
    d. Change VBIOS to 2162.
    e. Fixed system resume from USB device while select ACPI Sleep state to Disabled in setup menu.

  Release BIOS Information:
    A274X015.BIN --- System BIOS and fullsku Me.
    A274X015.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X014.bin ; A274X014.rom
  BIOS Checksum : 0xE5A5 ; 0x77A5
  BIOS String   : (A274X014.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/10

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Change "Restore AC Power Loss" Item value to "Power Off" as default.
    b. Hidden "High Precision Timer" string.
    c. Added Azlia control Item.
    d. Fixed USB keyboard/mouse can wake up from S4 while select ACPI Sleep state to S1 only.
    e. Added to support CaseOpen function.
    f. Added to Inform EC for system entry S1.
    g. Fixed TPM driver install fail issue.
    h. Fixed coding error for RTCstatescode eModule.

  Release BIOS Information:
    A274X014.BIN --- System BIOS and fullsku Me.
    A274X014.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X013.bin ; A274X013.rom
  BIOS Checksum : 0x70BB ; 0x20BB
  BIOS String   : (A274X013.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/2

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Modified BIOS Memory Informaiton & SETUP Items by DQA request.
    b. Update PCH code to limit USB keyboard/mouse wake up from S4.
    c. Modified some item for "LCD Control" page in BIOS Setup menu.
    d. Hidden CSM16 Parameters page.
    e. Hidden Toggle EC item.

  Release BIOS Information:
    A274X013.BIN --- System BIOS and fullsku Me.
    A274X013.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X012.bin ; A274X012.rom
  BIOS Checksum : 0x9700 ; 0x2900
  BIOS String   : (A274X012.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2013/1/2

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW017.

  Release BIOS Information:
    A274X012.BIN --- System BIOS and fullsku Me.
    A274X012.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X011.bin ; A274X011.rom
  BIOS Checksum : 0xAD53 ; 0xAB81
  BIOS String   : (A274X011.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/12/31

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Fixed typo error for "LVDS VESA\JEIDA Select" Item.
    b. Added "Backlight Signal Control" Item.
    c. Added to switch HD audio Verb Table by GPIO setting.
    d. System will be auto wakeup after RI# status active.

  Release BIOS Information:
    A274X011.BIN --- System BIOS and fullsku Me.
    A274X011.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X010.bin ; A274X010.rom
  BIOS Checksum : 0x0CC7 ; 0x0AF5
  BIOS String   : (A274X010.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/12/25

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Added to show system temperature in Setup menu.
    b. Added Wake on Ring function.
    c. Fixed PCI express by 16 can not work issue.
    d. Change "SATA Mode Selection" item value to "IDE" as default.
    e. Hidden "SATA test mode" Item.
    f. Enable Backlight control by PWM mode. (GPIO31 - High/Low : Linear/PWM)
    g. Added LVDS JEDIA /VESA selection.
    h. Modify SATA Port number from port 1 ~ port 6.
    i. Modify FAN speed string.
    j. Rewrite OememSmiCore.c.
    k. Added PCI Express Wake support.
    l. Modify Serial Port number to port 1 and port 2.

  Release BIOS Information:
    A274X010.BIN --- System BIOS and fullsku Me.
    A274X010.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X009.bin ; A274X009.rom
  BIOS Checksum : 0x4135 ; 0x3F63
  BIOS String   : (A274X009.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/12/21

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Fixed LAN1 will have a caution mark in device management after driver installed.
    b. Fixed can not detect COM1 device in device management. 

  Release BIOS Information:
    A274X009.BIN --- System BIOS and fullsku Me.
    A274X009.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X008.bin ; A274X008.rom
  BIOS Checksum : 0x1774 ; 0x15A2
  BIOS String   : (A274X008.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/12/13

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Fixed ITE8518 HWM show error issue (OBF report mistake).
    b. Change U2ECR(USB2.0 Electrical Control Register) default value.
    c. Add LAN1 ,LAN2 control and PXE OpRom setup item.

  Release BIOS Information:
    A274X008.BIN --- System BIOS and fullsku Me.
    A274X008.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X007.bin ; A274X007.rom
  BIOS Checksum : 0x9FEE ; 0x9E1C
  BIOS String   : (A274X007.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/12/4

  Owner         : Pat.Huang
  Requester     : Vicki.Tsai
  Customer      : Advantech

  Release Description:
    a. Change "XHCI Mode" item value to "Auto" as default to fix USB KB/MS work abnormal during install OS..
    b. Fixed PS2 KB/MS can not work under OS.
    c. Modify CH7511 LVDS panel string.
    d. Updated ME FW version to 9.0.0.1257.
    e. Updated codebase to Aptio 4.6.5.4_VEB_1AQQW016.

  Release BIOS Information:
    A274X007.BIN --- System BIOS and fullsku Me.
    A274X007.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X006.bin ; A274X006.rom
  BIOS Checksum : 0x7733 ; 0x159C
  BIOS String   : (A274X006.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/28

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    a. Updated HD audio Verb table.
    b. Added Serial IO Console Redirection support.
    c. Added for COM2 RS/232/RS422/RS485 support.
    d. Change "XHCI Mode" item value to "Enable" as default.
    e. Hidden "USB Ports Per-Port Disable Control" item.
    f. Hidden Un-use PCI-Express root port configuration.
    g. Hidden "Intel ICC" page.

  Release BIOS Information:
    A274X006.BIN --- System BIOS and fullsku Me.
    A274X006.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X005.bin ; A274X005.rom
  BIOS Checksum : 0x32F3 ; 0x70AB
  BIOS String   : (A274X005.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/27

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    a. Update ExternalObffEn of PwrOptConfig to disable. (Fixed system can not shutdown in DOS mode)
    b. Modify GPIO setting.
    c. Fixed system hang up at post code 0x05 while reset or shutdown.
    d. Added Fan2 support and modify HWM string.

  Release BIOS Information:
    A274X005.BIN --- System BIOS and fullsku Me.
    A274X005.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X004.bin ; A274X004.rom
  BIOS Checksum : 0x0573 ; 0xA3DC
  BIOS String   : (A274X004.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/23

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    a. Fixed Port80 can not display issue.
    b. Modify DIMM Spd address to fix system hang up at memory init.

  Release BIOS Information:
    A274X004.BIN --- System BIOS and fullsku Me.
    A274X004.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X003.bin ; A274X003.rom
  BIOS Checksum : 0x9047 ; 0x41B5
  BIOS String   : (A274X003.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/20

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    a. Added SIO ITE8518 emodule.
    b. Modify "SYSTEM Agent(SA) Configuration" page.
    c. Modify "PCH-IO Configuration" page.

  Release BIOS Information:
    A274X003.BIN --- System BIOS and fullsku Me.
    A274X003.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X002.bin ; A274X002.rom
  BIOS Checksum : 0xCB7C ; 0x7CEA
  BIOS String   : (A274X002.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/19

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    a. Hidden System Language item.
    b. Added Memory information in Main Page.
    c. Addec RTC status code to report CMOS checksum error.
    d. Added Resume from RTC support.
    e. Updated VBIOS for display issue.
    f. Added to sup[port CH7511 (DP to LVDS).
    g. Modify GPIO Setting.
    h. Modify PCIE clock setting.
    i. Hidden Thermal Configuration Page.
    j. Hidden Acoustic Management Configuraion Page.
    k. Hidden Smart Settings Page.
    l. Hidden Platform Misc Configuration Page.
    m. Hidden Intel RC Drivers Version Detail Page.

  Release BIOS Information:
    A274X002.BIN --- System BIOS and fullsku Me.
    A274X002.ROM --- System BIOS.


//----------------------------------------------------------------------------
//  Revision History
//----------------------------------------------------------------------------
  BIOS Name     : A274X001.bin ; A274X001.rom
  BIOS Checksum : 0x00EB ; 0x4DC3
  BIOS String   : (A274X001.BIN) EVALUATION FOR V1.10 - NOT FOR SALE!
  Release Date  : 2012/11/14

  Owner         : Pat.Huang
  Requester     : Jessica.Chen
  Customer      : Advantech

  Release Description:
    Bring up.

  Release BIOS Information:
    A274X001.BIN --- System BIOS and fullsku Me.
    A274X001.ROM --- System BIOS.
